{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":15,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-K / RX-K"]
[]
[]
[]
[]
["","","","","FTX20KV1B / RX20K2V1B","FTX20KV1B / RX20K5V1B","FTX25KV1B / RX25K2V1B","FTX25KV1B / RX25K5V1B","FTX35KV1B / RX35K2V1B","FTX35KV1B / RX35K5V1B","FTX50K2V1B / RX50K2V1B","FTX50KV1B / RX50KV1B","FTX60K2V1B / RX60K2V1B","FTX60KV1B / RX60KV1B","FTX71K2V1B / RX71K2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3","1.7","1.7","1.7","1.7","2.3"]
["","Max.","","kW","2.6","2.6","3.0","3.0","4.0","4.0","6.0","6.0","7.0","7.0","7.3"]
["","Nom.","","kW","2.0 (2)","2.0 (2)","2.5 (2)","2.5 (2)","3.5 (2)","3.5 (2)","5.0","5.0 (2)","6.0","6.0 (2)","7.1"]
["Space cooling","SEER","","","6.66","6.66","6.55","6.55","6.42","6.44","6.59","6.59","6.76","6.76","5.25"]
["","Annual energy consumption","","kWh/a","105","106","134","134","180","191","266","266","311","311","473"]
["","Capacity","Pdesign","kW","2.00","2.00","2.50","2.50","3.50","3.50","5.00","5.00","6.00","6.00","7.10"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.20","2.20","2.40","2.40","2.80","2.80","4.60","4.60","4.80","4.80","6.20"]
["","SCOP/A","","","4.65","4.65","4.61","4.61","4.64","4.64","4.10","4.10","4.10","4.10","3.81"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A+","A+","A+","A+","A"]
["","Annual energy consumption","","kWh/a","662","663","729","729","845","845","1,570","1,570","1,640","1,640","2,277"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","","6.35","","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5","","12.7","","12.7"]
["","Drain","OD","mm","18","18","18","18","18","18","","16","","16"]
["Nominal efficiency","EER","","","3.98 (1)","3.98 (1)","3.78 (1)","3.78 (1)","3.4 (1)","3.4 (1)","3.58","3.58 (1)","3.65","3.65 (1)","2.61"]
["","Annual energy consumption","","kWh","251","251","331","331","510","510","698","698","822","822","1,360"]
["","COP","","","4.77 (1)","4.77 (1)","4.36 (1)","4.36 (1)","4.0 (1)","4.0 (1)","3.80","3.80 (1)","3.63","3.63 (1)","3.19"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","","A","","A"]
["","","Heating","","A","A","A","A","A","A","","A","","A"]
["Heating capacity","Nom.","","kW","2.5 (2)","2.5 (2)","3.0 (2)","3.0 (2)","4.0 (2)","4.0 (2)","6.0","6.0 (2)","7.0","7.0 (2)","8.2"]
["","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3","1.7","1.7","1.7","1.7","2.3"]
["","Max.","","kW","3.5","3.5","4.0","4.0","4.8","4.8","7.7","7.7","8.0","8.0","9.0"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]