{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":22,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-KV / RX-K"]
[]
[]
[]
[]
["","","","","FTX20K2V1B / RX20K2V1B","FTX20K2V1B / RX20K5V1B9","FTX20K2V1B / RX20K5V1B","FTX20K5V1B / RX20K2V1B","FTX20K5V1B / RX20K5V1B9","FTX25K2V1B / RX25K2V1B","FTX25K2V1B / RX25K5V1B9","FTX25K2V1B / RX25K5V1B","FTX25K5V1B / RX25K2V1B","FTX25K5V1B / RX25K5V1B9","FTX35K2V1B / RX35K2V1B","FTX35K2V1B / RX35K5V1B9","FTX35K2V1B / RX35K5V1B","FTX35K5V1B / RX35K2V1B","FTX35K5V1B / RX35K5V1B9","FTX50KMV1B / RX50KV1B","FTX60KMV1B / RX60KV1B","FTX71KMV1B / RX71KV1B"]
["Cooling capacity","Min.","","kW","","","","1.3","1.3","","","","1.3","1.3","","","","1.3","1.3"]
["","Max.","","kW","","","","2.6","2.6","","","","3.0","3.0","","","","4.0","4.0"]
["","Nom.","","kW","2.0","2.0","2.0","2.00","2.00","2.5","2.5","2.5","2.50","2.50","3.5","3.5","3.5","3.50","3.50","5.0","6.0","7.1"]
["Space cooling","SEER","","","6.66","6.66","6.66","6.66","6.66","6.55","6.55","6.55","6.55","6.55","6.44","6.44","6.44","6.44","6.44","6.59","6.76","5.25"]
["","Annual energy consumption","","kWh/a","105","105","105","105","105","134","134","134","134","134","190","190","190","190","190","266","311","473"]
["","Capacity","Pdesign","kW","2.00","2.00","2.00","2.00","2.00","2.50","2.50","2.50","2.50","2.50","3.50","3.50","3.50","3.50","3.50","5.00","6.00","7.10"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.20","2.20","2.20","2.20","2.20","2.40","2.40","2.40","2.40","2.40","2.80","2.80","2.80","2.80","2.80","4.60","4.80","6.20"]
["","SCOP/A","","","4.65","4.65","4.65","4.65","4.65","4.61","4.61","4.61","4.61","4.61","4.64","4.64","4.64","4.64","4.64","4.10","4.10","3.81"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A+","A+","A"]
["","Pdh Heating capacity at -10°","","kW","","","","1.74","1.74","","","","1.85","1.85","","","","","2.17"]
["","Annual energy consumption","","kWh/a","662","662","662","662","662","729","729","729","729","729","845","845","845","845","845","1,570","1,640","2,277"]
["Nominal efficiency","EER","","","3.98","3.98","3.98","3.98","3.98","3.78","3.78","3.78","3.78","3.78","3.43","3.43","3.43","3.43","3.43","3.58","3.65","2.61"]
["","Annual energy consumption","","kWh","251","251","251","251","251","331","331","331","331","331","510","510","510","510","510","698","822","1,360"]
["","COP","","","4.77","4.77","4.77","4.77","4.77","4.36","4.36","4.36","4.36","4.36","4.02","4.02","4.02","4.02","4.02","3.80","3.63","3.19"]
["","Energy labeling Directive","Cooling","","","","","A","A","","","","A","A","","","","A","A"]
["","","Heating","","","","","A","A","","","","A","A","","","","A","A"]
["Heating capacity","Nom.","","kW","2.50","2.50","2.50","2.50","2.50","3.00","3.00","3.00","3.00","3.00","4.00","4.00","4.00","4.00","4.00","6.00","7.00","8.20"]
["","Min.","","kW","","","","1.30","1.30","","","","1.30","1.30","","","","1.30","1.30"]
["","Max.","","kW","","","","3.50","3.50","","","","4.00","4.00","","","","4.80","4.80"]
["Notes","","","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]