{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":10,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BT / RXA-A"]
[]
[]
[]
[]
["","","","","FTXA20B2V1BT / RXA20A5V1B","FTXA20B2V1BT / RXA20A3V1B","FTXA25B2V1BT / RXA25A3V1B","FTXA25B2V1BT / RXA25A5V1B","FTXA35B2V1BT / RXA35A5V1B","FTXA35B2V1BT / RXA35A3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","","1.4","1.4"]
["","Max.","","kW","2.6","2.6","3.2","","4.0","4.0"]
["","Nom.","","kW","2.0","2.0","2.5","","3.4","3.4"]
["Space cooling","SEER","","","8.75","8.75","8.74","","8.73","8.73"]
["","Annual energy consumption","","kWh/a","80","80","101","","137","137"]
["","Capacity","Pdesign","kW","2.00","2.00","2.50","","3.40","3.40"]
["","Energy efficiency class","","","A+++","A+++","A+++","","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.40","2.45","","2.50","2.50"]
["","SCOP/A","","","5.15","5.15","5.15","","5.15","5.15"]
["","Energy efficiency class","","","A+++","A+++","A+++","","A+++","A+++"]
["","Pdh Heating capacity at -10°","","kW","2.19","2.19","2.30","","2.36","2.36"]
["","Annual energy consumption","","kWh/a","653","653","666","","680","680"]
["Nominal efficiency","EER","","","4.70","4.70","4.46","","4.37","4.37"]
["","COP","","","5.00","5.00","5.00","","4.04","4.04"]
["","Energy labeling Directive","Cooling","","A","A","A","","A","A"]
["","","Heating","","A","A","A","","A","A"]
["Heating capacity","Nom.","","kW","2.50","2.50","2.80","","4.00","4.00"]
["","Min.","","kW","1.30","1.30","1.30","","1.40","1.40"]
["","Max.","","kW","3.50","3.50","4.70","","5.20","5.20"]
["Outdoor unit","","","","","RXA20A2V1B","RXA25A2V1B","RXA25A5V1B","","RXA35A2V1B"]
["Cooling capacity","Min.","","kW","","","","1.3"]
["","Nom.","","kW","","","","2.5"]
["","Max.","","kW","","","","3.2"]
["Heating capacity","Min.","","kW","","","","1.30"]
["","Nom.","","kW","","","","2.80"]
["","Max.","","kW","","","","4.70"]
["Nominal efficiency","EER","","","","","","4.46"]
["","COP","","","","","","5.00"]
["","Energy labeling Directive","Cooling","","","","","A"]
["","","Heating","","","","","A"]
["Space cooling","Energy efficiency class","","","","","","A+++"]
["","Capacity","Pdesign","kW","","","","2.50"]
["","SEER","","","","","","8.74"]
["","Annual energy consumption","","kWh/a","","","","101"]
["Space heating (Average climate)","Energy efficiency class","","","","","","A+++"]
["","Capacity","Pdesign","kW","","","","2.45"]
["","SCOP/A","","","","","","5.15"]
["","Pdh Heating capacity at -10°","","kW","","","","2.30"]
["","Annual energy consumption","","kWh/a","","","","666"]
["Energy Efficiency Range","","","","","","","A+++ ~ D"]