{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":10,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXB-C"]
[]
[]
[]
[]
["","","","","","FTXB20C2V1B","FTXB25C2V1B","FTXB35C2V1B","FTXB50CV1B","FTXB60CV1B"]
["Sound pressure level","Heating","","High","dBA","","","","40"]
["","","","Silent operation","dBA","","","","32"]
["","","","Low","dBA","","","","35"]
["","Cooling","","Silent operation","dBA","","","","32"]
["","","","Super high","dBA","","","","44"]
["","","","Low","dBA","","","","35"]
["","","","High","dBA","","","","40"]
["","","","Nom.","dBA","","","","38"]
["","Cooling","","Nom.","dBA","","","","38"]
["Control systems","Infrared remote control","","","","","","","AP GS02"]
["Piping connections","Drain","","","","","","","19.05"]
["Sound power level","Cooling","","","dBA","","","","55"]
["Dimensions","Unit","","Width","mm","","","","1,065"]
["","","","Depth","mm","","","","224"]
["","","","Height","mm","","","","310"]
["Casing","Colour","","","","","","","White"]
["Weight","Unit","","","kg","","","","14"]
["Power supply","Phase","","","","","","","1~"]
["","Name","","","","","","","V1"]
["","Frequency","","","Hz","","","","50"]
["","Voltage","","","V","","","","220-240"]
["Notes","","","","","","","","(1) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit)."]
["Power input","Cooling","","Nom.","kW","0.03","0.030","0.030"]
["","Heating","","Nom.","kW","0.04","0.040","0.040"]
["Casing","Colour","","","","White","White","White","","White"]
["Dimensions","Unit","","Height","mm","216","216","216","","310"]
["","","","Width","mm","770","770","770","","1065"]
["","","","Depth","mm","283","283","283","","224"]
["Weight","Unit","","","kg","8","8.00","8.00","","14"]
["Fan","Air flow rate","Cooling","High","m³/min","9.1","9.2","9.3","","18.5"]
["","","","Medium","m³/min","7.4","7.6","7.7"]
["","","","Low","m³/min","5.9","6.0","6.1","","14.34"]
["","","","Silent operation","m³/min","4.7","4.8","4.9","","12.36"]
["","","Heating","High","m³/min","9.4","9.7","10.1","","18.54"]
["","","","Medium","m³/min","7.8","8.0","8.4"]
["","","","Low","m³/min","6.3","6.3","6.7","","14.3"]
["","","","Silent operation","m³/min","5.5","5.5","5.7","","12.36"]
["Sound power level","Cooling","","","dBA","55","55","58","","61"]
["Sound pressure level","Cooling","","High","dBA","39","40","41","","43"]
["","","","Medium","dBA","33","33","34"]
["","","","Low","dBA","25","26","27","","37"]
["","","","Silent operation","dBA","21","21","23","","33"]
["","Heating","","High","dBA","39","40","41","","43"]
["","","","Medium","dBA","34","34","35"]
["","","","Low","dBA","28","28","29","","37"]
["","","","Silent operation","dBA","25","25","26","","33"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.50","9.50"]
["","Drain","","","","18","18","18","","19.05"]
["Control systems","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","","AP GS02"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Power supply","Name","","","","V1","V1","V1","","V1"]
["","Phase","","","","1~","1~","1~","","1~"]
["","Frequency","","","Hz","50","50","50","","50"]
["","Voltage","","","V","220-240","220-240","220-240","","220-240"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","","","","","16.56"]
["Sound pressure level","Cooling","","Nom.","dBA","","","","","41"]
["Fan","Air flow rate","Heating","Nom.","m³/min","","","","","16.56"]
["Sound pressure level","Heating","","Nom.","dBA","","","","","41"]
["","Cooling","","Super high","dBA","","","","","46"]