{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":12,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D / RXF-D"]
[]
[]
[]
[]
["","","","","FTXF20D5V1B / RXF20D5V1B","FTXF25D5V1B / RXF25D5V1B","FTXF35D5V1B / RXF35D5V1B","FTXF42D5V1B / RXF42D5V1B","FTXF50D2V1B / RXF50D5V1B","FTXF50D2V1B / RXF50D6V1B","FTXF60D2V1B / RXF60D5V1B","FTXF71D2V1B / RXF71D5V1B"]
["Outdoor unit","","","","RXF20D5V1B","RXF25D5V1B","RXF35D5V1B","RXF42D5V1B","RXF50D5V1B","","RXF60D5V1B","RXF71D5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.4","1.70","1.7","1.70","2.30"]
["","Nom.","","kW","2.00","2.50","3.30","4.20","5.00","5","6.00","7.10"]
["","Max.","","kW","2.4","2.8","3.8","4.3","6.00","6","7.00","7.30"]
["Heating capacity","Min.","","kW","1.30","1.30","1.30","1.40","1.70","1.7","1.70","2.30"]
["","Nom.","","kW","2.40","2.80","3.50","4.60","6.00","6","6.40","8.20"]
["","Max.","","kW","3.30","3.70","4.40","5.00","7.70","7.7","8.00","9.00"]
["Nominal efficiency","EER","","","3.38","3.24","3.30","3.30","3.33","3.33","3.25","2.56"]
["","COP","","","3.75","3.73","3.72","3.71","3.71","3.71","3.93","3.15"]
["","Annual energy consumption","","kWh","","","","","751","751","923","1387"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","E"]
["","","Heating","","A","A","A","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A"]
["","Capacity","Pdesign","kW","2.00","2.50","3.50","4.20","5.00","5","6.00","7.10"]
["","SEER","","","6.50","6.50","6.50","6.50","6.21","6.21","6.15","5.15"]
["","Annual energy consumption","","kWh/a","108","135","188","226","282","282","342","483"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+","A"]
["","Capacity","Pdesign","kW","2.20","2.40","2.60","3.30","4.60","4.6","4.80","6.20"]
["","SCOP/A","","","4.11","4.11","4.11","4.30","4.06","4.06","4.06","3.81"]
["","Pdh Heating capacity at -10°","","kW","1.91","2.00","2.22","2.61","4.07","4.07","4.24","5.02"]
["","Annual energy consumption","","kWh/a","749","818","885","1075","1585","1585","1654","2275"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]