{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LS"]
[]
[]
[]
[]
["","","","","","FTXG20LV1BS","FTXG25LV1BS","FTXG35LV1BS","FTXG50LV1BS"]
["Power input","Cooling","","Nom.","kW","0.023 (3) (1) (2), 0.023 (3) (1) (2), 0.023 (3) (1) (2)","0.023 (2) (1) (3), 0.023 (2) (1) (3), 0.023 (2) (1) (3)","0.033 (2) (3) (1), 0.033 (2) (3) (1), 0.033 (2) (3) (1)","0.033 (1) (2) (3), 0.033 (1) (2) (3), 0.033 (1) (2) (3)"]
["","Heating","","Nom.","kW","0.031 (1) (2) (3), 0.031 (1) (2) (3), 0.031 (1) (2) (3)","0.033 (1) (3) (2), 0.033 (1) (3) (2), 0.033 (1) (3) (2)","0.042 (2) (1) (3), 0.042 (2) (1) (3), 0.042 (2) (1) (3)","0.043 (1) (2) (3), 0.043 (1) (2) (3), 0.043 (1) (2) (3)"]
["Casing","Colour","","","","Silver","Silver","Silver","Silver"]
["Dimensions","Unit","","Height","mm","303","303","303","303"]
["","","","Width","mm","998","998","998","998"]
["","","","Depth","mm","212","212","212","212"]
["Weight","Unit","","","kg","12.0","12.0","12.0","12.0"]
["Fan","Air flow rate","Cooling","High","m³/min","8.9","8.9","10.9","10.9"]
["","","","Medium","m³/min","6.6","6.6","7.8","8.9"]
["","","","Low","m³/min","4.4","4.4","4.8","6.8"]
["","","","Silent operation","m³/min","2.6","2.6","2.9","3.6"]
["","","Heating","High","m³/min","10.2","11.0","12.4","12.6"]
["","","","Medium","m³/min","8.4","8.6","9.6","10.5"]
["","","","Low","m³/min","6.3","6.3","6.9","8.1"]
["","","","Silent operation","m³/min","3.8","3.8","4.1","5.0"]
["Sound power level","Cooling","","","dBA","54","54","59","60"]
["","Heating","","","dBA","56","56","59","60"]
["Sound pressure level","Cooling","","High","dBA","38","38","45","46"]
["","","","Medium","dBA","32","32","34","40"]
["","","","Low","dBA","25","25","26","35"]
["","","","Silent operation","dBA","19","19","20","25"]
["","Heating","","High","dBA","40","41","45","47"]
["","","","Medium","dBA","34","34","37","41"]
["","","","Low","dBA","28","28","29","35"]
["","","","Silent operation","dBA","19","19","20","25"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.50","9.50","9.50","12.7"]
["","Drain","","","","18","18","18","18"]
["Control systems","Infrared remote control","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Batteries","","","","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Power supply","Name","","","","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]