{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV"]
[]
[]
[]
[]
["","","","","","FTXL25J2V1B","FTXL35J2V1B"]
["Power input","Cooling","","Nom.","kW","0.040 (1) (2) (3), 0.040 (1) (2) (3), 0.040 (1) (2) (3)","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)"]
["","Heating","","Nom.","kW","0.040 (1) (2) (3), 0.040 (1) (2) (3), 0.040 (1) (2) (3)","0.040 (3) (2) (1), 0.040 (3) (2) (1), 0.040 (3) (2) (1)"]
["Casing","Colour","","","","White","White"]
["Dimensions","Unit","","Height","mm","283","283"]
["","","","Width","mm","770","770"]
["","","","Depth","mm","198","198"]
["Weight","Unit","","","kg","8.00","8.00"]
["Fan","Air flow rate","Cooling","High","m³/min","9.3","9.3"]
["","","","Medium","m³/min","7.7","7.7"]
["","","","Low","m³/min","6.1","6.1"]
["","","","Silent operation","m³/min","4.9","4.9"]
["","","Heating","High","m³/min","10.1","10.1"]
["","","","Medium","m³/min","8.4","8.4"]
["","","","Low","m³/min","6.7","6.7"]
["","","","Silent operation","m³/min","5.7","5.7"]
["Sound power level","Cooling","","","dBA","57","57"]
["","Heating","","","dBA","57","57"]
["Sound pressure level","Cooling","","High","dBA","41","41"]
["","","","Medium","dBA","34","34"]
["","","","Low","dBA","27","27"]
["","","","Silent operation","dBA","23","23"]
["","Heating","","High","dBA","41","41"]
["","","","Medium","dBA","35","35"]
["","","","Low","dBA","29","29"]
["","","","Silent operation","dBA","26","26"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","9.50","9.50"]
["","Drain","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC433A87, ARC466A9","ARC433A87, ARC466A9"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Batteries","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Power supply","Name","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]
["","","","","","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]