{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / RXM-M9"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / RXM20M3V1B9","FTXM25N2V1B / RXM25M3V1B9","FTXM35N2V1B / RXM35M3V1B9"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.4"]
["","Max.","","kW","2.6","3.2","4.0"]
["","Nom.","","kW","2.0","2.5","3.4"]
["Space cooling","SEER","","","8.53","8.52","8.51"]
["","Annual energy consumption","","kWh/a","83","103","140"]
["","Capacity","Pdesign","kW","2.00","2.50","3.40"]
["","Energy efficiency class","","","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.30","2.40","2.50"]
["","SCOP/A","","","5.10","5.10","5.10"]
["","Energy efficiency class","","","A+++","A+++","A+++"]
["","Pdh Heating capacity at -10°","","kW","2.24","2.30","2.35"]
["","Annual energy consumption","","kWh/a","632","659","686"]
["Nominal efficiency","Annual energy consumption","","kWh","220","280","400"]
["","EER","","","4.57","4.50","4.23"]
["","COP","","","5.00","5.00","4.04"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Heating capacity","Nom.","","kW","2.50","2.80","4.00"]
["","Min.","","kW","1.30","1.30","1.40"]
["","Max.","","kW","3.50","4.70","5.20"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]