{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / RXM-N"]
[]
[]
[]
[]
["","","","","FTXM42N2V1B / RXM42N2V1B","FTXM50N2V1B / RXM50N2V1B","FTXM60N2V1B / RXM60N2V1B","FTXM71N2V1B / RXM71N2V1B"]
["Cooling capacity","Min.","","kW","1.70","1.70","1.90","2.30"]
["","Max.","","kW","5.00","5.30","6.70","8.50"]
["","Nom.","","kW","4.20","5.00","6.00","7.10"]
["Space cooling","SEER","","","7.50","7.33","6.90","6.20"]
["","Annual energy consumption","","kWh/a","196","239","304","401"]
["","Capacity","Pdesign","kW","4.20","5.00","6.00","7.10"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.00","4.60","4.60","6.20"]
["","SCOP/A","","","4.60","4.60","4.30","4.10"]
["","Energy efficiency class","","","A++","A++","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","3.68","4.09","4.09","5.01"]
["","Annual energy consumption","","kWh/a","1,216","1,400","1,496","2,115"]
["Nominal efficiency","Annual energy consumption","","kWh","","","","1,172"]
["","EER","","","3.75","3.68","3.39","3.03"]
["","COP","","","4.12","4.00","3.61","3.19"]
["","Energy labeling Directive","Cooling","","A","A","A","B"]
["","","Heating","","A","A","A","D"]
["Heating capacity","Nom.","","kW","5.40","5.80","7.00","8.20"]
["","Min.","","kW","1.70","1.70","1.70","2.30"]
["","Max.","","kW","6.00","6.50","8.00","10.20"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for operation range"]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]