{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":16,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 5XXM-A"]
[]
[]
[]
[]
["","","","","FTXM20R2V1B / FTXM20R2V1B / FTXM25R2V1B / 5XXM68A2V1B","FTXM20R2V1B / FTXM25R2V1B / FTXM25R2V1B / 5XXM68A2V1B","FTXM20R2V1B / FTXM50R2V1B / 5XXM68A2V1B","FTXM25R2V1B / FTXM42R2V1B / 5XXM68A2V1B","FTXM35R2V1B / FTXM35R2V1B / 5XXM68A2V1B","FTXM20R2V1B / FTXM71R2V1B / 5XXM90A2V1B","FTXM42R2V1B / FTXM50R2V1B / 5XXM90A2V1B","FTXM20R2V1B / FTXM20R2V1B / FTXM50R2V1B / 5XXM90A2V1B","FTXM20R2V1B / FTXM25R2V1B / FTXM42R2V1B / 5XXM90A2V1B","FTXM20R2V1B / FTXM35R2V1B / FTXM35R2V1B / 5XXM90A2V1B","FTXM25R2V1B / FTXM25R2V1B / FTXM42R2V1B / 5XXM90A2V1B","FTXM20R2V1B / FTXM20R2V1B / FTXM25R2V1B / FTXM25R2V1B / 5XXM90A2V1B"]
["Cooling capacity","Nom.","","kW","6.50","6.80","6.80","6.70","6.80","8.00","8.00","8.00","8.00","8.00","8.00","7.80"]
["Heating capacity","Nom.","","kW","8.00","8.50","8.40","8.10","8.40","10.00","10.00","10.00","10.00","10.00","10.00","10.00"]
["Nominal efficiency","EER","","","3.62","3.48","2.95","2.94","2.91","2.87","2.77","3.29","3.24","3.29","3.29","3.71"]
["","COP","","","3.74","3.64","3.22","3.24","3.07","3.27","3.23","3.65","3.61","3.49","3.65","4.01"]
["","Annual energy consumption","","kWh","898","977","1153","1139","1168","1394","1444","1216","1235","1216","1216","1051"]
["","Energy labeling Directive","Cooling","","A","A","C","C","C","C","D","A","A","A","A","A"]
["","","Heating","","A","A","C","C","D","C","C","A","A","B","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","6.50","6.80","6.80","6.70","6.80","8.00","8.00","8.00","8.00","8.00","8.00","7.80"]
["","SEER","","","7.29","7.18","6.74","6.77","6.68","6.58","6.50","7.05","7.03","7.04","7.04","7.50"]
["","Annual energy consumption","","kWh/a","312","332","353","346","356","426","431","397","399","398","397","364"]
["Space heating (Average climate)","Energy efficiency class","","","A","A","A","A","A","A+","A","A+","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","5.30","5.30","4.50","4.30","4.80","4.50","5.20","6.46","5.60","6.46","5.60","6.46"]
["","SCOP/A","","","3.88","3.91","3.87","3.85","3.82","4.08","3.98","4.16","4.22","4.07","4.25","4.41"]
["","Pdh Heating capacity at -10°","","kW","3.77","3.77","3.23","3.06","3.45","3.24","3.72","4.63","4.01","4.65","4.02","4.64"]
["","Annual energy consumption","","kWh/a","1912","1900","1628","1565","1760","1544","1829","2172","1857","2225","1846","2051"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB.","(1) - Inlet/outlet water temperature 7/12 °C; inlet air temperature 27°C DB 19°C WB."]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for operation range","(4) - See separate drawing for operation range","(4) - See separate drawing for operation range","(4) - See separate drawing for operation range","(4) - See separate drawing for operation range","(4) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]