{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":19,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-R"]
[]
[]
[]
[]
["","","","","FTXM20R5V1B / RXM20R5V1B","FTXM20R2V1B / RXM20R5V1B","FTXM25R5V1B / RXM25R5V1B","FTXM25R2V1B / RXM25R5V1B","FTXM35R5V1B / RXM35R5V1B","FTXM35R2V1B / RXM35R5V1B","FTXM42R2V1B / RXM42R5V1B","FTXM42R2V1B / RXM42R2V1B","FTXM42R5V1B / RXM42R5V1B","FTXM42R5V1B / RXM42R2V1B","FTXM50R2V1B / RXM50R2V1B","FTXM50R2V1B / RXM50R5V1B","FTXM60R2V1B / RXM60R2V1B","FTXM60R2V1B / RXM60R5V1B","FTXM71R2V1B / RXM71R2V1B"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.30","1.30","1.40","1.40","","","","","","","","","2.30"]
["","Nom.","","kW","2.00","2.00","2.50","2.50","3.40","3.40","","","","","","","","","7.10"]
["","Max.","","kW","2.60","2.60","3.20","3.20","4.00","4.00","","","","","","","","","8.50"]
["Heating capacity","Min.","","kW","1.30","1.30","1.30","1.30","1.40","1.40","","","","","","","","","2.30"]
["","Nom.","","kW","2.50","2.50","2.80","2.80","4.00","4.00","","","","","","","","","8.20"]
["","Max.","","kW","3.50","3.50","4.70","4.70","5.20","5.20","","","","","","","","","10.20"]
["Nominal efficiency","Annual energy consumption","","kWh","219","219","278","278","402","402","","","","","","","","","1,172"]
["","COP","","","5.00","5.00","5.00","5.00","4.04","4.04","","","","","","","","","3.19"]
["","EER","","","4.57","4.57","4.50","4.50","4.23","4.23","","","","","","","","","3.03"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","","","","","","","","","B"]
["","","Heating","","A","A","A","A","A","A","","","","","","","","","D"]
["Space cooling","Annual energy consumption","","kWh/a","81","81","101","101","137","137","","","","","","","","","401"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","","","","","","","","","A++"]
["","Capacity","Pdesign","kW","2.00","2.00","2.50","2.50","3.40","3.40","","","","","","","","","7.10"]
["","SEER","","","8.65","8.65","8.65","8.65","8.65","8.65","","","","","","","","","6.20"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","631","631","659","659","686","686","","","","","","","","","2,117"]
["","Capacity","Pdesign","kW","2.30","2.30","2.40","2.40","2.50","2.50","","","","","","","","","6.20"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","","","","","","","","","A+"]
["","Pdh Heating capacity at -10°","","kW","2.24","2.24","2.30","2.30","2.35","2.35","","","","","","","","","5.01"]
["","SCOP/A","","","5.10","5.10","5.10","5.10","5.10","5.10","","","","","","","","","4.10"]
["Notes","","","","","(1) - See separate drawing for operation range","","(1) - See separate drawing for operation range","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","","(2) - See separate drawing for electrical data","","(2) - See separate drawing for electrical data","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Min.","","kW","","","","","","","1.7","1.7","1.7","1.7","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","","","","","","","4.2","4.2","4.2","4.2","5","5","6","6"]
["","Max.","","kW","","","","","","","5","5","5","5","6","6","7","7"]
["Heating capacity","Min.","","kW","","","","","","","1.7","1.7","1.7","1.7","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","","","","","","","5.4","5.4","5.4","5.4","5.8","5.8","7","7"]
["","Max.","","kW","","","","","","","6","6","6","6","7.7","7.7","8","8"]
["Nominal efficiency","EER","","","","","","","","","4.33","4.33","4.33","4.33","3.68","3.68","3.39","3.39"]
["","COP","","","","","","","","","4.12","4.12","4.12","4.12","4","4","3.61","3.61"]
["","Annual energy consumption","","kWh","","","","","","","485","485","485","485","679","679","885","885"]
["","Energy labeling Directive","Heating","","","","","","","","A","A","A","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","","","","","","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","","","4.2","4.2","4.2","4.2","5","5","6","6"]
["","SEER","","","","","","","","","7.85","7.85","7.85","7.85","7.41","7.41","6.9","6.9"]
["","Annual energy consumption","","kWh/a","","","","","","","187","187","187","187","236","236","304","304"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","A++","A++","A++","A++","A++","A++","A+","A+"]
["","Capacity","Pdesign","kW","","","","","","","4","4","4","4","4.6","4.6","4.8","4.8"]
["","SCOP/A","","","","","","","","","4.71","4.71","4.71","4.71","4.71","4.71","4.3","4.3"]
["","Pdh Heating capacity at -10°","","kW","","","","","","","3.67","3.67","3.67","3.67","3.85","3.85","3.99","3.99"]
["","Annual energy consumption","","kWh/a","","","","","","","1189","1189","1189","1189","1368","1368","1562","1562"]
["Nominal efficiency","Energy labeling Directive","Cooling","","","","","","","","","","","","A","A","A","A"]