{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":16,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R"]
[]
[]
[]
[]
["","","","","","FTXM20R2V1B","FTXM20R5V1B","FTXM25R2V1B","FTXM25R5V1B","FTXM35R5V1B","FTXM35R2V1B","FTXM42R2V1B","FTXM42R5V1B","FTXM50R2V1B","FTXM60R2V1B","FTXM71R2V1B"]
["Power input","Cooling","","Nom.","kW","0.029","0.029","0.025","0.025","0.03","0.03","0.034","0.034","0.03","0.032","0.054"]
["","Heating","","Nom.","kW","0.023","0.023","0.022","0.022","0.027","0.027","0.038","0.038","0.032","0.035","0.06"]
["Casing","Colour","","","","White","White","White","White","White","White","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","295","295","295","295","295","295","295","295","299","299","299"]
["","","","Width","mm","778","778","778","778","778","778","778","778","998","998","998"]
["","","","Depth","mm","272","272","272","272","272","272","272","272","292","292","292"]
["Weight","Unit","","","kg","10","10","10","10","10","10","10","10","14.5","14.5","14.5"]
["Fan","Air flow rate","Cooling","High","m³/min","10.5","10.5","10.5","10.5","11.3","11.3","11.9","11.9","15.8","16.7","16.9"]
["","","","Medium","m³/min","7.5","7.5","7.6","7.6","7.8","7.8","9","9","14","14","15"]
["","","","Low","m³/min","5.7","5.7","5.7","5.7","6","6","6.5","6.5","11.4","11.8","12.2"]
["","","","Silent operation","m³/min","4.3","4.3","4.1","4.1","4.2","4.2","4.3","4.3","8.3","9.1","10"]
["","","Heating","High","m³/min","9.3","9.3","9.8","9.8","9.8","9.8","12.4","12.4","15.8","16.5","17.7"]
["","","","Medium","m³/min","8.2","8.2","8","8","8.5","8.5","9.7","9.7","14.2","15.2","15.8"]
["","","","Low","m³/min","6.2","6.2","6.3","6.3","6.5","6.5","6.5","6.5","12","12.4","12.7"]
["","","","Silent operation","m³/min","5.1","5.1","4.9","4.9","4.9","4.9","4.9","4.9","10.5","11.1","11.6"]
["Sound power level","Cooling","","","dBA","57","57","57","57","58","58","60","60","58","60","60"]
["","Heating","","","dBA","54","54","54","54","54","54","60","60","58","59","61"]
["Sound pressure level","Cooling","","High","dBA","41","41","41","41","45","45","45","45","44","46","47"]
["","","","Medium","dBA","33","33","33","33","33","33","39","39","40","42","43"]
["","","","Low","dBA","25","25","25","25","29","29","30","30","36","37","38"]
["","","","Silent operation","dBA","19","19","19","19","19","19","21","21","27","30","32"]
["","Heating","","High","dBA","39","39","39","39","39","39","45","45","43","45","46"]
["","","","Medium","dBA","34","34","34","34","35","35","39","39","39","41","42"]
["","","","Low","dBA","26","26","27","27","28","28","29","29","34","36","37"]
["","","","Silent operation","dBA","20","20","20","20","20","20","21","21","31","33","34"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5","9.5","9.5","12.7","12.7","15.9"]
["","Drain","","","","18","18","18","18","18","18","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1","1","1","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1","1","1"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Power supply","Name","","","","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(1) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(1) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["Standard Accessories","Silver particle filter","","","","","","","","","","","","1","1","1"]