{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-K3 / RXP-K3"]
[]
[]
[]
[]
["","","","","FTXP20K3V1B / RXP20K3V1B","FTXP25K3V1B / RXP25K3V1B","FTXP35K3V1B / RXP35K3V1B","FTXP50K3V1B / RXP50K3V1B","FTXP60K3V1B / RXP60K3V1B","FTXP71K3V1B / RXP71K3V1B"]
["Outdoor unit","","","","RXP20K3V1B","RXP25K3V1B","RXP35K3V1B","RXP50K3V1B","RXP60K3V1B","RXP71K3V1B"]
["Cooling capacity","Nom.","","kW","2.00","2.50","3.50","5.0","6.0","7.1"]
["Heating capacity","Nom.","","kW","2.50","3.00","4.00","6.0","7.0","8.2"]
["Nominal efficiency","EER","","","4.02","3.83","3.48","3.61","3.29","2.64"]
["","COP","","","4.77","4.36","4.02","3.80","3.63","3.19"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","D"]
["","","Heating","","A","A","A","A","A","D"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++","A"]
["","Capacity","Pdesign","kW","2.00","2.50","3.50","5.00","6.00","7.10"]
["","SEER","","","6.79","6.92","6.64","6.72","6.82","5.30"]
["","Annual energy consumption","","kWh/a","103","126","185","260","308","469"]
["Space heating (Average climate)","Energy efficiency class","","","A++","A++","A++","A+","A+","A"]
["","Capacity","Pdesign","kW","2.20","2.40","2.80","4.60","4.80","6.20"]
["","SCOP/A","","","4.65","4.61","4.64","4.10","4.10","3.81"]
["","Pdh Heating capacity at -10°","","kW","2","2","2","4.07","4.12","4.89"]
["","Annual energy consumption","","kWh/a","662","728","845","1571","1640","2279"]
["Notes","","","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]