{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":16,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-L / RXP-L"]
[]
[]
[]
[]
["","","","","FTXP20L2V1B / RXP20L5V1B","FTXP20L5V1B / RXP20L5V1B","FTXP20L2V1B / RXP20L2V1B","FTXP25L2V1B / RXP25L5V1B","FTXP25L5V1B / RXP25L5V1B","FTXP25L2V1B / RXP25L2V1B","FTXP35L2V1B / RXP35L2V1B","FTXP35L2V1B / RXP35L5V1B","FTXP35L5V1B / RXP35L5V1B","FTXP50L2V1B / RXP50L2V1B","FTXP60L2V1B / RXP60L2V1B","FTXP71L2V1B / RXP71L2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","","1.3","1.3","","1.3","1.3","1.3","","","2.3"]
["","Max.","","kW","2.6","2.6","","3.0","3.0","","4.0","4.0","4.0","","","7.3"]
["","Nom.","","kW","2.00","2.00","","2.50","2.50","","3.50","3.50","3.50","","","7.1"]
["Nominal efficiency","EER","","","4.02","4.02","","3.83","3.83","","3.49","3.49","3.49","","","2.64"]
["","Annual energy consumption","","kWh","","","","","","","","","","","","1,345"]
["","COP","","","4.77","4.77","","4.36","4.36","","4.02","4.02","4.02","","","3.19"]
["","Energy labeling Directive","Cooling","","A","A","","A","A","","A","A","A"]
["","","Heating","","A","A","","A","A","","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","","104","","","127","","186","","186","","","469"]
["","Capacity","Pdesign","kW","","2.00","","","2.50","","3.50","","3.50","","","7.10"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","2.20","","","2.40","","2.80","","2.80","","","6.20"]
["","Pdh Heating capacity at -10°","","kW","","1.99","","","2.10","","","","2.33","","","5.02"]
["","Annual energy consumption","","kWh/a","","662","","","728","","845","","845","","","2,278"]
["Heating capacity","Nom.","","kW","2.50","2.50","","3.00","3.00","","4.00","4.00","4.00","","","8.2"]
["","Min.","","kW","1.30","1.30","","1.30","1.30","","1.30","1.30","1.30","","","2.3"]
["","Max.","","kW","3.50","3.50","","4.00","4.00","","4.80","4.80","4.80","","","9.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]
["Space cooling","SEER","","","","6.79","","","6.92","","6.62","","6.62","","","5.30"]
["","Energy efficiency class","","","","A++","","","A++","","A++","","A++","","","A"]
["Space heating (Average climate)","SCOP/A","","","","4.65","","","4.61","","4.64","","4.64","","","3.81"]
["","Energy efficiency class","","","","A++","","","A++","","A++","","A++","","","A"]
["Outdoor unit","","","","","","RXP20L2V1B","","","RXP25L2V1B"]
["Cooling capacity","Min.","","kW","","","1.3","","","1.3","","","","1.7","1.7"]
["","Nom.","","kW","","","2.00","","","2.50","","","","5.0","6.0"]
["","Max.","","kW","","","2.6","","","3.0","","","","6.0","7.0"]
["Heating capacity","Min.","","kW","","","1.30","","","1.30","","","","1.7","1.7"]
["","Nom.","","kW","","","2.50","","","3.00","","","","6.0","7.0"]
["","Max.","","kW","","","3.50","","","4.00","","","","7.70","8.00"]
["Nominal efficiency","EER","","","","","4.02","","","3.83","","","","3.61","3.29"]
["","COP","","","","","4.77","","","4.36","","","","3.80","3.63"]
["","Energy labeling Directive","Cooling","","","","A","","","A"]
["","","Heating","","","","A","","","A"]
["Space cooling","Energy efficiency class","","","","","A++","","","A++","","","","A++","A++"]
["","Capacity","Pdesign","kW","","","2.00","","","2.50","","","","5.00","6.00"]
["","SEER","","","","","6.79","","","6.92","","","","6.72","6.82"]
["","Annual energy consumption","","kWh/a","","","104","","","127","","","","261","308"]
["Space heating (Average climate)","Energy efficiency class","","","","","A++","","","A++","","","","A+","A+"]
["","Capacity","Pdesign","kW","","","2.20","","","2.40","","","","4.60","4.80"]
["","SCOP/A","","","","","4.65","","","4.61","","","","4.10","4.10"]
["","Pdh Heating capacity at -10°","","kW","","","1.99","","","2.10","","","","4.12","4.24"]
["","Annual energy consumption","","kWh/a","","","662","","","728","","","","1570","1637"]
["Energy Efficiency Range","","","","","","A+++ ~ D","","","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D"]
["Nominal efficiency","Annual energy consumption","","kWh","","","","","","","","","","693","912"]