{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-L / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP35L2V1B / RXP35M5V1B","FTXP35L5V1B / RXP35M5V1B","FTXP50L2V1B / RXP50M2V1B","FTXP60L2V1B / RXP60M2V1B","FTXP71L2V1B / RXP71M2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.7","1.7","2.3"]
["","Max.","","kW","4.0","4.0","6.0","7.0","7.3"]
["","Nom.","","kW","3.50","3.50","5.0","6.0","7.1"]
["Space cooling","SEER","","","6.62","6.62","6.72","6.82","5.30"]
["","Annual energy consumption","","kWh/a","186","186","261","308","469"]
["","Capacity","Pdesign","kW","3.50","3.50","5.00","6.00","7.10"]
["","Energy efficiency class","","","A++","A++","A++","A++","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.80","2.80","4.60","4.80","6.20"]
["","SCOP/A","","","4.64","4.64","4.10","4.10","3.81"]
["","Energy efficiency class","","","A++","A++","A+","A+","A"]
["","Pdh Heating capacity at -10°","","kW","2.33","2.33","4.12","4.24","5.02"]
["","Annual energy consumption","","kWh/a","845","845","1,570","1,637","2,278"]
["Nominal efficiency","Annual energy consumption","","kWh","","","693","912","1,345"]
["","EER","","","3.49","3.49","3.61","3.29","2.64"]
["","COP","","","4.02","4.02","3.80","3.63","3.19"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","4.00","4.00","6.0","7.0","8.2"]
["","Min.","","kW","1.30","1.30","1.7","1.7","2.3"]
["","Max.","","kW","4.80","4.80","7.70","8.00","9.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]