{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Cooling capacity","Nom.","","kW","4"]
["Heating capacity","Nom.","","kW","4.2"]
["Nominal efficiency","EER","","","3.71"]
["","COP","","","3.75"]
["","Annual energy consumption","","kWh","539"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Space cooling","Energy efficiency class","","","A++"]
["","Capacity","Pdesign","kW","4"]
["","SEER","","","7.74"]
["","Annual energy consumption","","kWh/a","181"]
["Space heating (Average climate)","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","3.2"]
["","SCOP/A","","","4.3"]
["","Pdh Heating capacity at -10°","","kW","2.46"]
["","Annual energy consumption","","kWh/a","1041"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","4.00"]
["Heating capacity","Nom.","","kW","","5.20"]
["Nominal efficiency","Annual energy consumption","","kWh","","554"]
["","COP","","","","3.68"]
["","EER","","","","3.61"]
["","Energy labeling Directive","Cooling","","","A"]
["","","Heating","","","A"]
["Space cooling","Annual energy consumption","","kWh/a","","188"]
["","Energy efficiency class","","","","A++"]
["","Capacity","Pdesign","kW","","4.00"]
["","SEER","","","","7.45"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","","1,357"]
["","Capacity","Pdesign","kW","","4.00"]
["","Energy efficiency class","","","","A+"]
["","Pdh Heating capacity at -10°","","kW","","2.62"]
["","SCOP/A","","","","4.13"]