{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":12,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.4","7.1","7.7","7.7","8.6","16.0","17.2"]
["Sound pressure level","Cooling","","Nom.","dBA","32","32","34","38","39","41","42"]
["Fan","Air flow rate","Heating","Nom.","m³/min","8.2","7.9","8.5","9.4","9.3","14.9","16.7"]
["Sound pressure level","Heating","","Nom.","dBA","33","34","36","38","39","40","42"]
["Power input","Cooling","","Nom.","kW","","","","","","0.040 (3) (2) (4), 0.040 (3) (2) (4), 0.040 (3) (2) (4)","0.045 (3) (4) (2), 0.045 (3) (4) (2), 0.045 (3) (4) (2)"]
["","Heating","","Nom.","kW","","","","","","0.045 (4) (3) (2), 0.045 (4) (3) (2), 0.045 (4) (3) (2)","0.060 (2) (3) (4), 0.060 (2) (3) (4), 0.060 (2) (3) (4)"]
["Casing","Colour","","","","White","White","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","295","295","295","295","295","290","290"]
["","","","Width","mm","800","800","800","800","800","1050","1050"]
["","","","Depth","mm","215","215","215","215","215","250","250"]
["Weight","Unit","","","kg","9","9","10","10","10","12","12"]
["Fan","Air flow rate","Cooling","High","m³/min","9.4","9.1","10.4","9.1","10.2","16.0","17.2"]
["","","","Low","m³/min","5.5","5.2","4.8","6.3","7.0","11.3","11.5"]
["","","","Silent operation","m³/min","4.0","3.7","3.5","5.4","6.0","10.1","10.5"]
["","","Heating","High","m³/min","9.9","9.8","10.6","11.2","11.0","17.2","19.5"]
["","","","Low","m³/min","6.5","6.2","6.4","7.7","7.6","12.6","14.2"]
["","","","Silent operation","m³/min","5.5","5.2","5.4","6.8","6.7","11.3","12.6"]
["Sound power level","Cooling","","","dBA","54","54","58","58","59","60","63"]
["","Heating","","","dBA","54","55","58","58","60","59","62"]
["Sound pressure level","Cooling","","High","dBA","38","38","42","42","43","45","46"]
["","","","Low","dBA","25","25","26","33","34","36","37"]
["","","","Silent operation","dBA","22","22","23","30","31","33","34"]
["","Heating","","High","dBA","38","39","42","42","44","44","46"]
["","","","Low","dBA","28","28","29","33","34","35","37"]
["","","","Silent operation","dBA","25","25","26","30","31","32","34"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","9.52","9.52","9.52","12.70","12.7","15.9"]
["","Drain","","","","18","18","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","","","","","","ARC452A3","ARC452A3"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Batteries","","","","2","2","2","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2","2","2","2","2","2"]
["Power supply","Name","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 230V"]
["","","","","","","","","","","(4) - 240V","(4) - 240V"]
["Standard Accessories","Titanium apatite photocatalytic air purification filter without frame","","","","","","","","","","2"]