{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R / RXTM-N"]
[]
[]
[]
[]
["","","","","FTXTM30R2V1B / RXTM30N2V1B","FTXTM40R2V1B / RXTM40N2V1B"]
["Cooling capacity","Min.","","kW","0.70","0.90"]
["","Max.","","kW","4.50","5.10"]
["","Nom.","","kW","3.00","4.00"]
["Space cooling","SEER","","","7.60","7.70"]
["","Annual energy consumption","","kWh/a","138","182"]
["","Capacity","Pdesign","kW","3.00","4.00"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.00","3.80"]
["","SCOP/A","","","5.12","5.30"]
["","Energy efficiency class","","","A+++","A+++"]
["","Pdh Heating capacity at -10°","","kW","3.00","3.80"]
["","Annual energy consumption","","kWh/a","821","1,003"]
["Nominal efficiency","Annual energy consumption","","kWh","366","539"]
["","EER","","","4.10","3.71"]
["","COP","","","5.34","5.37"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","3.20","4.00"]
["","Min.","","kW","0.80","1.20"]
["","Max.","","kW","6.70","7.20"]
["Notes","","","","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]