{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K / RXTP-N"]
[]
[]
[]
[]
["","","","","FTXTP35K3V1B / RXTP35N2V1B","FTXTP25K3V1B / RXTP25N2V1B"]
["Cooling capacity","Min.","","kW","0.70","0.70"]
["","Max.","","kW","4.40","4.00"]
["","Nom.","","kW","3.50","2.50"]
["Space cooling","SEER","","","7.20","7.10"]
["","Annual energy consumption","","kWh/a","170","123"]
["","Capacity","Pdesign","kW","3.50","2.50"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.00","2.50"]
["","SCOP/A","","","4.81","4.98"]
["","Energy efficiency class","","","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","3.00","2.50"]
["","Annual energy consumption","","kWh/a","873","703"]
["Nominal efficiency","EER","","","3.80","4.40"]
["","Annual energy consumption","","kWh","460","285"]
["","COP","","","4.44","4.95"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","4.00","3.20"]
["","Min.","","kW","0.80","0.80"]
["","Max.","","kW","6.70","6.20"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]"]
["","","","","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]