{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":7,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-M"]
[]
[]
[]
[]
["","","","","","FTXTP25M5V1B","FTXTP35M5V1B"]
["Power input","Cooling","","Nom.","kW","0.032","0.032"]
["","Heating","","Nom.","kW","0.032","0.032"]
["Casing","Colour","","","","White","White"]
["Dimensions","Unit","","Height","mm","286","286"]
["","","","Width","mm","770","770"]
["","","","Depth","mm","225","225"]
["Weight","Unit","","","kg","9","9"]
["Fan","Air flow rate","Cooling","High","m³/min","11.5","11.5"]
["","","","Medium","m³/min","8.3","8.3"]
["","","","Low","m³/min","5.5","5.5"]
["","","","Silent operation","m³/min","3.9","3.9"]
["","","Heating","High","m³/min","11.5","11.5"]
["","","","Medium","m³/min","8.7","8.7"]
["","","","Low","m³/min","5.6","5.6"]
["","","","Silent operation","m³/min","4.5","4.5"]
["Sound power level","Cooling","","","dBA","58","58"]
["","Heating","","","dBA","58","58"]
["Sound pressure level","Cooling","","High","dBA","43","43"]
["","","","Medium","dBA","35","35"]
["","","","Low","dBA","26","26"]
["","","","Silent operation","dBA","21","21"]
["","Heating","","High","dBA","43","43"]
["","","","Medium","dBA","35","35"]
["","","","Low","dBA","26","26"]
["","","","Silent operation","dBA","21","21"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5"]
["","Drain","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC480A53","ARC480A53"]
["","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]