{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZAG71M7V1B","FUA71AVEB / RZAG71M7V1B","FUA100AVEB / RZAG100M7V1B","FUA71AVEB / FUA71AVEB / RZAG100M7V1B","FUA125AVEB / RZAG125M7V1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","12.1 (1)"]
["Space cooling","SEER","","","6.89","7.02","6.42","8.82","6.39"]
["","Annual energy consumption","","kWh/a","345","339","518","377","1,136"]
["","Capacity","Pdesign","kW","6.80","6.80","9.50","9.50","12.1"]
["","Energy efficiency class","","","A++","A++","A++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.70","4.70","7.80","7.80","9.52"]
["","SCOP/A","","","4.28","4.20","4.50","4.73","4.26"]
["","Energy efficiency class","","","A+","A+","A+","A++"]
["","Annual energy consumption","","kWh/a","1,537","1,567","2,427","2,309","3,129"]
["Heating capacity","Nom.","","kW","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","13.5 (2)"]
["Notes","","","","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data"]