{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":69,"n_cols":11,"rows_kept":69,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB","FUA71AVEB9","FUA100AVEB","FUA100AVEB9","FUA125AVEB","FUA125AVEB9"]
["Sound pressure level","Heating","","High","dBA","41","","46","","47"]
["","","","Medium","dBA","38","","42","","43"]
["","","","Low","dBA","35","","39","","40"]
["","Cooling","","Medium","dBA","38","","42","","43"]
["","","","Low","dBA","35","","39","","40"]
["","","","High","dBA","41","","46","","47"]
["Standard Accessories","Operation manual","","","","1","1","1","1","1","1"]
["","Installation manual","","","","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1"]
["","Thermal insulation tube","","","","3","3","3","3","3","3"]
["","Tie-wraps","","","","10","10","10","10","10","10"]
["","Hose band","","","","1","1","1","1","1","1"]
["","Sealing material","","","","4","4","4","4","4","4"]
["","Washer fixing plate","","","","1","1","1","1","1","1"]
["","Drain joint","","","","1","1","1","1","1","1"]
["","Non woven fabric","","","","1","1","1","1","1","1"]
["","Washer","","","","8","8","8","8","8","8"]
["","Fixing screw for drain hose","","","","5","5","5","5","5","5"]
["Control systems","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Cooling capacity","Total capacity","","Nom.","kW","","","","","12.1"]
["Piping connections","Liquid","","OD","mm","9.52","","9.52","","9.52"]
["","Gas","","OD","mm","15.9","","15.9","","15.9"]
["","Drain","","","","VP25 (OD Ø32.0)","","VP25 (OD Ø32.0)","","VP25 (OD Ø32.0)"]
["Sound power level","Cooling","","","dBA","59","","64","","65"]
["","Heating","","","dBA","59","","64"]
["Dimensions","Unit","","Width","mm","950","","950","","950"]
["","","","Depth","mm","950","","950","","950"]
["","","","Height","mm","198","","198","","198"]
["Casing","Material","","","","Resin","","Resin","","Resin"]
["","Colour","","","","Fresh White","","Fresh White","","Fresh White"]
["Weight","Unit","","","kg","25.0","","26.0","","26"]
["Fan","Air flow rate","Heating","High","m³/min","23.0","","31.0","","32.5"]
["","","","Medium","m³/min","19.5","","25.5","","26.5"]
["","","","Low","m³/min","16.0","","20.0","","20.5"]
["","","Cooling","Low","m³/min","16.0","","20.0","","20.5"]
["","","","Medium","m³/min","19.5","","25.5","","26.5"]
["","","","High","m³/min","23.0","","31.0","","32.5"]
["Drain-up height","mm","","","","600","600","600","600","600","600"]
["Heating capacity","Total capacity","","Nom.","kW","","","","","13.5"]
["Casing","Colour","","","","","Fresh White","","Fresh White","","Fresh White"]
["","Material","","","","","Resin","","Resin","","Resin"]
["Dimensions","Unit","","Height","mm","","198","","198","","198"]
["","","","Width","mm","","950","","950","","950"]
["","","","Depth","mm","","950","","950","","950"]
["Weight","Unit","","","kg","","25.0","","26.0","","26.0"]
["Fan","Air flow rate","Cooling","High","m³/min","","23.0","","31.0","","32.5"]
["","","","Medium","m³/min","","19.5","","25.5","","26.5"]
["","","","Low","m³/min","","16.0","","20.0","","20.5"]
["","","Heating","High","m³/min","","23.0","","31.0","","32.5"]
["","","","Medium","m³/min","","19.5","","25.5","","26.5"]
["","","","Low","m³/min","","16.0","","20.0","","20.5"]
["Sound power level","Cooling","","","dBA","","59","","64","","65"]
["Sound pressure level","Cooling","","High","dBA","","41","","46","","47"]
["","","","Medium","dBA","","38","","42","","43"]
["","","","Low","dBA","","35","","39","","40"]
["","Heating","","High","dBA","","41","","46","","47"]
["","","","Medium","dBA","","38","","42","","43"]
["","","","Low","dBA","","35","","39","","40"]
["Piping connections","Liquid","","OD","mm","","9.52","","9.52","","9.52"]
["","Gas","","OD","mm","","15.9","","15.9","","15.9"]
["","Drain","","","","","VP25 (OD Ø32.0)","","VP25 (OD Ø32.0)","","VP25 (OD Ø32.0)"]
["Cooling capacity","Total capacity","","Nom.","kW","","","","","","12.10"]
["Heating capacity","Total capacity","","Nom.","kW","","","","","","13.5"]