{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MY"]
[]
[]
[]
[]
["","","","","FVA125AMVEB / RZASG125MUY","FVA140AMVEB / RZASG140MUY","FVA71AMVEB / FVA71AMVEB / RZASG140MUY"]
["Cooling capacity","Nom.","","kW","12.1 (1)","13.4 (1)","13.4 (1)"]
["Heating capacity","Nom.","","kW","13.5 (2)","15.5 (2)","15.5 (2)"]
["Space cooling","Capacity","Pdesign","kW","12.1","13.4","13.4"]
["","SEER","","","5.52","5.63","7.71"]
["","Annual energy consumption","","kWh/a","1314","1429","1043"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6","7.8","7.8"]
["","SCOP/A","","","3.64","3.81","4.43"]
["","Annual energy consumption","","kWh/a","2308","2866","2467"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]