{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":12,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A / RXM-R"]
[]
[]
[]
[]
["","","","","FVXM25A2V1B / RXM25R5V1B","FVXM25A3V1B / RXM25R5V1B","FVXM35A2V1B / RXM35R5V1B","FVXM35A3V1B / RXM35R5V1B","FVXM50A2V1B / RXM50R2V1B","FVXM50A2V1B / RXM50R5V1B","FVXM50A3V1B / RXM50R2V1B","FVXM50A3V1B / RXM50R5V1B"]
["Cooling capacity","Min.","","kW","1.30","","1.40","","1.40","1.40"]
["","Max.","","kW","3.50","","4.00","","5.80","5.80"]
["","Nom.","","kW","2.40","","3.40","","5.00","5.00"]
["Space cooling","SEER","","","8.55","","8.11","","7.30","7.30"]
["","Annual energy consumption","","kWh/a","98","","147","","240","240"]
["","Capacity","Pdesign","kW","2.40","","3.40","","5.00","5.00"]
["","Energy efficiency class","","","A+++","","A++","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.30","","2.80","","4.10","4.10"]
["","SCOP/A","","","4.65","","4.63","","4.31","4.31"]
["","Energy efficiency class","","","A++","","A++","","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","2.03","","2.34","","3.58","3.58"]
["","Annual energy consumption","","kWh/a","693","","847","","1,330","1,330"]
["Nominal efficiency","Annual energy consumption","","kWh","268","","424","","656","656"]
["","EER","","","4.47","","4.01","","3.81","3.81"]
["","COP","","","4.55","","3.90","","3.81","3.81"]
["","Energy labeling Directive","Cooling","","A","","A","","A","A"]
["","","Heating","","A","","A","","A","A"]
["Heating capacity","Nom.","","kW","3.40","","4.50","","5.80","5.80"]
["","Min.","","kW","1.30","","1.40","","1.40","1.40"]
["","Max.","","kW","4.70","","5.80","","8.10","8.10"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Min.","","kW","","1.30","","1.40","","","1.40","1.40"]
["","Nom.","","kW","","2.40","","3.40","","","5.00","5.00"]
["","Max.","","kW","","3.50","","4.00","","","5.80","5.80"]
["Heating capacity","Min.","","kW","","1.30","","1.40","","","1.40","1.40"]
["","Nom.","","kW","","3.40","","4.50","","","5.80","5.80"]
["","Max.","","kW","","4.70","","5.80","","","8.10","8.10"]
["Nominal efficiency","EER","","","","4.47","","4.01","","","3.81","3.81"]
["","COP","","","","4.55","","3.90","","","3.81","3.81"]
["","Annual energy consumption","","kWh","","268","","424","","","656","656"]
["","Energy labeling Directive","Cooling","","","A","","A","","","A","A"]
["","","Heating","","","A","","A","","","A","A"]
["Space cooling","Energy efficiency class","","","","A+++","","A++","","","A++","A++"]
["","Capacity","Pdesign","kW","","2.40","","3.40","","","5.00","5.00"]
["","SEER","","","","8.55","","8.11","","","7.30","7.30"]
["","Annual energy consumption","","kWh/a","","98","","147","","","240","240"]
["Space heating (Average climate)","Energy efficiency class","","","","A++","","A++","","","A+","A+"]
["","Capacity","Pdesign","kW","","2.30","","2.80","","","4.10","4.10"]
["","SCOP/A","","","","4.65","","4.63","","","4.31","4.31"]
["","Pdh Heating capacity at -10°","","kW","","2.03","","2.34","","","3.58","3.58"]
["","Annual energy consumption","","kWh/a","","693","","847","","","1,330","1,330"]