{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A / RXM-R9"]
[]
[]
[]
[]
["","","","","FVXM25A2V1B / RXM25R5V1B9","FVXM25A3V1B / RXM25R5V1B9","FVXM35A2V1B / RXM35R5V1B9","FVXM35A3V1B / RXM35R5V1B9"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.40","1.40"]
["","Max.","","kW","3.50","3.50","4.00","4.00"]
["","Nom.","","kW","2.40","2.40","3.40","3.40"]
["Space cooling","SEER","","","8.55","8.55","8.11","8.11"]
["","Annual energy consumption","","kWh/a","98","98","147","147"]
["","Capacity","Pdesign","kW","2.40","2.40","3.40","3.40"]
["","Energy efficiency class","","","A+++","A+++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.30","2.30","2.80","2.80"]
["","SCOP/A","","","4.65","4.65","4.63","4.63"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.03","2.03","2.34","2.34"]
["","Annual energy consumption","","kWh/a","693","693","847","847"]
["Nominal efficiency","Annual energy consumption","","kWh","268","268","424","424"]
["","EER","","","4.47","4.47","4.01","4.01"]
["","COP","","","4.55","4.55","3.90","3.90"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.40","3.40","4.50","4.50"]
["","Min.","","kW","1.30","1.30","1.40","1.40"]
["","Max.","","kW","4.70","4.70","5.80","5.80"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]