{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B / RXM-R"]
[]
[]
[]
[]
["","","","","FVXM50B2V1B / RXM50R2V1B","FVXM50B2V1B / RXM50R5V1B"]
["Cooling capacity","Min.","","kW","1.4","1.4"]
["","Nom.","","kW","5","5"]
["","Max.","","kW","5.8","5.8"]
["Heating capacity","Min.","","kW","1.4","1.4"]
["","Nom.","","kW","5.8","5.8"]
["","Max.","","kW","8.1","8.1"]
["Nominal efficiency","EER","","","3.81","3.81"]
["","COP","","","3.81","3.81"]
["","Annual energy consumption","","kWh","656","656"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++"]
["","Capacity","Pdesign","kW","5","5"]
["","SEER","","","7.3","7.3"]
["","Annual energy consumption","","kWh/a","240","240"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+"]
["","Capacity","Pdesign","kW","4.1","4.1"]
["","SCOP/A","","","4.31","4.31"]
["","Pdh Heating capacity at -10°","","kW","3.58","3.58"]
["","Annual energy consumption","","kWh/a","1,330","1,330"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]