{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":12,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-F / RXM-N9"]
[]
[]
[]
[]
["","","","","FVXM25FV1B / RXM25N2V1B9","FVXM25FV1B / RXM25N5V1B9","FVXM25FV1B9 / RXM25N2V1B9","FVXM35FV1B / RXM35N2V1B9","FVXM35FV1B / RXM35N5V1B9","FVXM35FV1B9 / RXM35N2V1B9","FVXM50FV1B / RXM50N2V1B9","FVXM50FV1B9 / RXM50N2V1B9"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.30","1.40","1.40","1.40","1.40","1.40"]
["","Max.","","kW","3.00","3.00","3.00","3.80","3.80","3.80","5.60","5.60"]
["","Nom.","","kW","2.50","2.50","2.50","3.50","3.50","3.50","5.00","5.00"]
["Space cooling","SEER","","","7.20","7.20","7.20","6.43","6.43","6.43","6.80","6.80"]
["","Annual energy consumption","","kWh/a","120","120","120","190","190","190","257","257"]
["","Capacity","Pdesign","kW","2.50","2.50","2.50","3.50","3.50","3.50","5.00","5.00"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.40","2.40","2.90","2.90","2.90","4.20","4.20"]
["","SCOP/A","","","4.56","4.56","4.56","4.00","4.00","4.00","4.00","4.00"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","2.23","2.23","","2.40","2.40","","2.23","2.23"]
["","Annual energy consumption","","kWh/a","737","737","737","1,015","1,015","1,015","1,471","1,471"]
["Nominal efficiency","EER","","","4.20","4.20","4.20","3.21","3.21","3.21","3.23","3.23"]
["","Annual energy consumption","","kWh","298","298","298","545","545","545","773","773"]
["","COP","","","4.42","4.42","4.42","3.78","3.78","3.78","3.63","3.63"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.40","3.40","3.40","4.50","4.50","4.50","5.80","5.80"]
["","Min.","","kW","1.30","1.30","1.30","1.40","1.40","1.40","1.40","1.40"]
["","Max.","","kW","4.50","4.50","4.50","5.00","5.00","5.00","8.10","8.10"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]