{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXL-M3"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXL25M3V1B","FVXS35FV1B / RXL35M3V1B"]
["Cooling capacity","Nom.","","kW","2.5","3.5"]
["Space cooling","SEER","","","5.10","5.21"]
["","Annual energy consumption","","kWh/a","173","235"]
["","Capacity","Pdesign","kW","2.50","3.50"]
["","Energy efficiency class","","","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.90","3.20"]
["","SCOP/A","","","4.01","3.77"]
["","Energy efficiency class","","","A+","A"]
["","Annual energy consumption","","kWh/a","1,012","1,187"]
["Nominal efficiency","EER","","","3.38","3.27"]
["","Annual energy consumption","","kWh","370","535"]
["","COP","","","3.78","3.46"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","B"]
["Heating capacity","Nom.","","kW","4.5","5.6"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - For rated minimal heating capacity indoor unit fan set to SL tap","(6) - For rated minimal heating capacity indoor unit fan set to SL tap"]
["","","","","(7) - Maximum heating capacity at -15°C outdoor temperature","(7) - Maximum heating capacity at -15°C outdoor temperature"]