{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F"]
[]
[]
[]
[]
["","","","","FVXS25FV1B","FVXS35FV1B","FVXS50FV1B"]
["Sound pressure level","Heating","High","dBA","38","39","45"]
["","","Silent operation","dBA","23","24","32"]
["","","Low","dBA","26","27","36"]
["","Cooling","Silent operation","dBA","23","24","32"]
["","","Low","dBA","26","27","36"]
["","","High","dBA","38","39","44"]
["","","Nom.","dBA","32","33","40"]
["","Cooling","Nom.","dBA","32","33","40"]
["Standard Accessories","Installation manual","","","1","1","1"]
["","Operation manual","","","1","1","1"]
["","Wireless remote control","","","1","1","1"]
["","Batteries","","","2","2","2"]
["","Remote control holder","","","1","1","1"]
["","Drain hose","","","1","1","1"]
["","Air purification filter","","","2"]
["","Thermal insulation tape","","","2","2","2"]
["Control systems","Infrared remote control","","","ARC452A1","ARC452A1","ARC452A1"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.52","12.7"]
["","Drain","","","20","20","20"]
["Sound power level","Cooling","","dBA","52","52","60"]
["","Heating","","dBA","52","52","60"]
["Dimensions","Unit","Width","mm","700","700","700"]
["","","Depth","mm","210","210","210"]
["","","Height","mm","600","600","600"]
["Casing","Colour","","","White","White","White"]
["Weight","Unit","","kg","14","14","14"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","V1","V1","V1"]
["","Frequency","","Hz","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240"]
["Notes","","","","(1) - 220V","(1) - 220V"]
["","","","","(2) - 230V","(2) - 230V"]
["","","","","(3) - 240V","(3) - 240V"]
["","","","","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["Standard Accessories","Air supply filter","","","","1","1"]