{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A"]
[]
[]
[]
[]
["","","","","","FVXTM30A3V1B"]
["Power input","Cooling","","Nom.","kW","0.02"]
["","Heating","","Nom.","kW","0.03"]
["Casing","Colour","","","","White"]
["Dimensions","Unit","","Height","mm","600"]
["","","","Width","mm","750"]
["","","","Depth","mm","238"]
["Weight","Unit","","","kg","17"]
["Fan","Air flow rate","Cooling","High","m³/min","9"]
["","","","Medium","m³/min","6.7"]
["","","","Low","m³/min","4.8"]
["","","","Silent operation","m³/min","4"]
["","","Heating","High","m³/min","9.4"]
["","","","Medium","m³/min","6.8"]
["","","","Low","m³/min","5.3"]
["","","","Silent operation","m³/min","4"]
["Sound power level","Cooling","","","dBA","53"]
["","Heating","","","dBA","53"]
["Sound pressure level","Cooling","","High","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","20"]
["","Heating","","High","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","19"]
["Refrigerant","GWP","","","","675"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.5"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC466A66"]
["","Wired remote control","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","2"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]