{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":39,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","GM"]
[]
[]
[]
[]
["","","","","","BGM0870Y1AA","MGM10326E","MGM103EA11XA","MGM10526E","MGM105EA11XA","MGM10626E","MGM106EA11XA","MGM10726E","MGM10726Y","MGM107EA11XA","MGM11026E","MGM110EA11XA","BGM110DA11XA","BGM11226Y","BGM112DA11XA","BGM117DA11XA","MGM1280Y1AA","MGM21126E","MGM211EA11XA","MGM21227E","MGM21227Y","MGM212EB11XA","MGM21327E","MGM213EB11XA","BGM218DA11XA","BGM220DB11XA","MGM2210Y1AA","MGM31527E","MGM315EB11XA","MGM32027E","MGM320EB11XA","BGM320DB11XA","BGM330DB11XA","BGM340DB11XA"]
["Refrigerant","GWP","","","","3","1,430","1,430","1,430","1,430","1,430","1,430","1,430","3","1,430","1,430","1,430","2,141","3","2,141","2,141","3","1,430","1,430","1,430","3","1,430","1,430","1,430","2,141","2,141","3","1,430","1,430","1,430","1,430","2,140","2,141"]
["","Type","","","","R-290","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-290","R-134a","R-134a","R-134a","R-452A","R-290","R-452A","R-452A","R-290","R-134a","R-134a","R-134a","R-290","R-134a","R-134a","R-134a","R-452A","R-452A","R-290","R-134a","R-134a","R-134a","R-134a","R-452A","R-452A"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","0.855 (1)","0.855","0.978 (1)","0.978 (1)","1.120 (1)","1.120 (1)","1.315 (1)","","1.315 (1)","1.351 (1)","1.351 (1)","","","","","","1.806 (1)","1.806 (1)","2.034 (1)","","2.034 (1)","2.175 (1)","2.175 (1)","","","","3.079 (1)","3.079 (1)","3.351 (1)","3.351 (1)"]
["","","R-290","Nom","kW","","","","","","","","","1.190 (1)","","","","","","","","1.281","","","","2.092 (1)","","","","","","2.206 (1)"]
["","Low temperature","R-290","Nom","kW","0.871 (1)","","","","","","","","","","","","","0.871 (1)"]
["","","R-452A","Nom","kW","","","","","","","","","","","","","0.679 (1)","","0.889 (1)","1.080 (1)","","","","","","","","","1.336 (1)","1.688 (1)","","","","","","2.491","2.349 (1)"]
["Operation range","Cold room temperature","","Min.","°C","","-5","-5","-5","-5","-5","-5","-5","-5","-5","-5","-5","-25","-25","-25","-25","","-5","-5","-5","-5","-5","-5","-5","-25","-25","","-5","-5","-5","-5","-25","-25"]
["","","","Max.","°C","","10","10","10","10","10","10","10","10","10","10","10","-15","-15","-15","-15","","10","10","10","10","10","10","10","-15","-15","","10","10","10","10","-15","-15"]
["Defrost","","","","","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","","Hot gas","Hot gas","Hot gas","Hot gas","","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas"]
["Dimensions","Unit","","Width","mm","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","400","620","620","620","620","620","620","620","620","620","620","620","620","620","620","620","620"]
["","","","Depth","mm","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","790","862","862","862","862","862","862"]
["","","","Height","mm","735","735","735","735","735","735","735","735","735","735","735","735","735","735","735","735","735","830","830","830","830","830","830","830","830","830","830","830","830","830","830","830","830"]
["Compressor","Nominal power","","","kW","0.9","0.4","0.4","0.5","0.5","0.4","0.4","0.7","","0.7","0.9","0.9","0.74","","0.9","1.3","0.56","0.9","0.9","1.7","","1.7","2","2","1.3","1.5","0.9","2.2","2.2","2.6","2.6","1.5","2.2"]
["","Type","","","","Hermetic","Hermetic Reciprocating","Hermetic","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic","Hermetic Reciprocating"]
["","Starting method","","","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","","Direct","Direct","Direct","Direct","","Direct","Direct","Direct","Direct","Direct","Direct","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct"]
["Weight","Unit","","","kg","64","52","52","53","53","56","56","56","56","56","64","64","56","64","64","64","56","80","80","80","80","80","80","80","80","80","80","98","98","100","100","105","105"]
["Condenser","Air flow","","","m³/h","","600","600","600","600","600","600","600","","600","600","600","600","","600","600","","1,200","1,200","1,200","","1,200","1,200","1,200","1,200","1,200","","1,500","1,500","1,500","1,500","1,500","1,500"]
["Evaporator","Air flow","","","m³/h","","600","600","600","600","600","600","600","","600","600","600","600","","600","600","","1,200","1,200","1,200","","1,200","1,200","1,200","1,200","1,200","","1,800","1,800","1,800","1,800","1,800","1,500"]
["","Air throw","","","m","4","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","","4 (2)","4 (2)","4 (2)","4 (2)","","4 (2)","4 (2)","4","4 (2)","4 (2)","4 (2)","","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4","10 (2)","10 (2)","10 (2)","10 (2)","10 (2)","10 (2)"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","3N~","1~","3N~","3N~","3N~","1~","3N~","1~","3N~","3N~","3N~","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","400","230","400","400","400","230","400","230","400","400","400","400","400","400"]
["Notes","","","","","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C"]
["","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]
["","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","(3) - Contains fluorinated greenhouse gases"]
["Refrigerating capacity","Low temperature","R-452A","Nom","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","3.16"]
["Dimensions","Unit","","Height","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","830"]
["","","","Width","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","620"]
["","","","Depth","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","1024"]
["Weight","Unit","","","kg","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","113"]
["Compressor","Type","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","Hermetic"]
["","Starting method","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","Direct"]
["Condenser","Air flow","","","m³/h","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","2200"]
["Evaporator","Air throw","","","m","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","10 (2)"]
["Operation range","Cold room temperature","","Min.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","-25"]
["","","","Max.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","-15"]
["Refrigerant","Type","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","R-452A"]
["","GWP","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","2140"]
["Power supply","Phase","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","3N~"]