{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":49,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","GS"]
[]
[]
[]
[]
["","","","","","BGS320DB13XXA","BGS320DB13XXB","BGS340DB13XXA","BGS340DB13XXB","MGS103EA12XXA","MGS103EA12XXB","MGS105EA12XXA","MGS105EA12XXB","MGS106EA12XXA","MGS106EA12XXB","MGS107EA12XXA","MGS107EA12XXB","BGS110DA12XXA","BGS110DA12XXB","MGS110EA12XXA","MGS110EA12XXB","SB.BGS11226D","BGS112DA12XXA","BGS112DA12XXB","SB.BGS11726D","BGS117DA12XXA","BGS117DA12XXB","SB.MGS21126E","MGS211EA12XXA","MGS211EA12XXB","SB.MGS21227E","MGS212EB12XXA","MGS212EB12XXB","SB.MGS21327E","SB.BGS21826D","BGS218DA12XXA","BGS218DA12XXB","SB.BGS22027D","BGS220DB12XXA","BGS220DB12XXB","SB.MGS31527E","MGS315EB13XXA","MGS315EB13XXB","SB.MGS32027E","MGS320EB13XXA","MGS320EB13XXB","SB.BGS33027D","BGS330DB13XXA","BGS330DB13XXB"]
["Refrigerant","GWP","","","","","","","","","","","","","","","","","","","","2,141","","","2,141","","","1,430","","","1,430","","","1,430","2,141","","","2,141","","","1,430","","","1,430","","","2,141"]
["","Type","","","","","","","","","","","","","","","","","","","","R-452A","","","R-452A","","","R-134a","","","R-134a","","","R-134a","R-452A","","","R-452A","","","R-134a","","","R-134a","","","R-452A"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","","","","","","","","","","","","","","","","","","","","","","1.806 (1)","","","2.034 (1)","","","2.175 (1)","","","","","","","3.079 (1)","","","3.351 (1)"]
["","Low temperature","R-452A","Nom","kW","","","","","","","","","","","","","","","","","0.889 (1)","","","1.080 (1)","","","","","","","","","","1.336 (1)","","","1.688 (1)","","","","","","","","","2.349 (1)"]
["Operation range","Cold room temperature","","Min.","°C","","","","","","","","","","","","","","","","","-25","","","-25","","","-5","","","-5","","","-5","-25","","","-25","","","-5","","","-5","","","-25"]
["","","","Max.","°C","","","","","","","","","","","","","","","","","-15","","","-15","","","10","","","10","","","10","-15","","","-15","","","10","","","10","","","-15"]
["Defrost","","","","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Hot gas","Electric","","Hot gas","Electric","","Electric","Electric","","Electric","Electric","","Electric","Hot gas","Electric","","Hot gas","Electric","","Electric","Electric","","Electric","Electric","","Hot gas","Electric"]
["Dimensions","Evaporator unit","","Depth","mm","","","","","","","","","","","","","","","","","410","","","410","","","410","","","410","","","410","410","","","410","","","410","","","410","","","410"]
["","","","Height","mm","","","","","","","","","","","","","","","","","215","","","215","","","215","","","215","","","215","215","","","215","","","215","","","215","","","215"]
["","","","Width","mm","","","","","","","","","","","","","","","","","654","","","654","","","1,074","","","1,074","","","1,074","1,074","","","1,074","","","1,654","","","1,654","","","1,654"]
["","Condensing unit","","Depth","mm","","","","","","","","","","","","","","","","","280","","","280","","","280","","","280","","","280","280","","","280","","","350","","","350","","","350"]
["","","","Width","mm","","","","","","","","","","","","","","","","","400","","","400","","","620","","","620","","","620","620","","","620","","","620","","","620","","","620"]
["Compressor","Nominal power","","","kW","","","","","","","","","","","","","","","","","0.9","","","1.3","","","0.9","","","1.7","","","2","1.3","","","1.5","","","2.2","","","2.6","","","2.2"]
["","Type","","","","","","","","","","","","","","","","","","","","Hermetic Reciprocating","","","Hermetic Reciprocating","","","Hermetic Reciprocating","","","Hermetic Reciprocating","","","Hermetic Reciprocating","Hermetic Reciprocating","","","Hermetic Reciprocating","","","Hermetic Reciprocating","","","Hermetic Reciprocating","","","Hermetic Reciprocating"]
["","Starting method","","","","","","","","","","","","","","","","","","","","Direct","","","Direct","","","Direct","","","Direct","","","Direct","Direct","","","Direct","","","Direct","","","Direct","","","Direct"]
["Condenser","Air flow","","","m³/h","","","","","","","","","","","","","","","","","600","","","600","","","1,200","","","1,200","","","1,200","1,200","","","1,200","","","1,500","","","1,500","","","1,500"]
["Evaporator","Air flow","","","m³/h","","","","","","","","","","","","","","","","","600","","","600","","","1,200","","","1,200","","","1,200","1,200","","","1,200","","","1,800","","","1,800","","","1,800"]
["","Air throw","","","m","","","","","","","","","","","","","","","","","4 (2)","","","4 (2)","","","4 (2)","","","4 (2)","","","4 (2)","4 (2)","","","4 (2)","","","4 (2)","","","4 (2)","","","4 (2)"]
["Defrost heaters","W","","","","1400","","3300","","450","","450","","450","","450","","450","","450","","450","450","","450","450","","800","800","","800","800","","800","800","800","","800","800","","1,400","1400","","1,400","1400","","1,400","1400"]
["Power supply","Phase","","","","","","","","","","","","","","","","","","","","1~","","","1~","","","1~","","","3N~","","","3N~","1~","","","3N~","","","3N~","","","3N~","","","3N~"]
["","Frequency","","","Hz","","","","","","","","","","","","","","","","","50","","","50","","","50","","","50","","","50","50","","","50","","","50","","","50","","","50"]
["","Voltage","","","V","","","","","","","","","","","","","","","","","230","","","230","","","230","","","400","","","400","230","","","400","","","400","","","400","","","400"]
["Refrigerating capacity","Low temperature","R-452A","Nom","kW","2.491","","3.16","","","","","","","","","","0.679","","","","","0.889","","","1.155","","","","","","","","","","1.429","","","1.688","","","","","","","","","2.701"]
["Casing","Colour","","Condensing unit","","Grey","White","Grey","White","Grey","White","Grey","White","Grey","White","Grey","White","Grey","White","Grey","White","","Grey","White","","Grey","White","","Grey","White","","Grey","White","","","Grey","White","","Grey","White","","Grey","White","","Grey","White","","Grey","White"]
["Dimensions","Condensing unit","","Width","mm","620","","620","","400","","400","","400","","400","","400","","400","","","400","","","400","","","620","","","620","","","","620","","","620","","","620","","","620","","","620"]
["","","","Depth","mm","350","","410","","280","","280","","280","","280","","280","","280","","","280","","","280","","","280","","","280","","","","280","","","280","","","350","","","350","","","350"]
["Compressor","Quantity","","","","1","","1","","1","","1","","1","","1","","1","","1","","","1","","","1","","","1","","","1","","","","1","","","1","","","1","","","1","","","1"]
["","Type","","","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","","Hermetic","","","Hermetic","","","Hermetic","","","Hermetic","","","","Hermetic","","","Hermetic","","","Hermetic","","","Hermetic","","","Hermetic"]
["","Model","","","","TFH2511Z/T","","NTZ096A4B","","NEU6212Z","","NEU6214Z","","NJ6220Z","","NTU6222ZV","","NEU2178GK","","NJ6226Z","","","NJ2192GJ","","","NJ2212GK/CSR","","","NJ6226Z","","","TFH4518Y/T","","","","NJ2212GK","","","TFH2480Z/T","","","TFH4525Y/T","","","MTZ40JH4","","","NTZ068A4B"]
["","Starting method","","","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","","Direct","","","Direct","","","Direct","","","Direct","","","","Direct","","","Direct","","","Direct","","","Direct","","","Direct"]
["Condenser","Air flow","","","m³/h","1500","","2200","","600","","600","","600","","600","","600","","600","","","600","","","600","","","1200","","","1200","","","","1200","","","1200","","","1500","","","1500","","","1500"]
["Operation range","Cold room temperature","","Min.","°C","-25","","-25","","-5","","-5","","-5","","-5","","-25","","-5","","","-25","","","-25","","","-5","","","-5","","","","-25","","","-25","","","-5","","","-5","","","-25"]
["","","","Max.","°C","-15","","-15","","10","","10","","10","","10","","-15","","10","","","-15","","","-15","","","10","","","10","","","","-15","","","-15","","","10","","","10","","","-15"]
["","Ambient temperature","","Min.","°C","20","","20","","20","","20","","20","","20","","20","","20","","","20","","","20","","","20","","","20","","","","20","","","20","","","20","","","20","","","20"]
["","","","Max.","°C","45","","45","","45","","45","","45","","45","","45","","45","","","45","","","45","","","45","","","45","","","","45","","","45","","","45","","","45","","","45"]
["Refrigerant","Type","","","","R-452A","","R-452A","","R-134a","","R-134a","","R-134a","","R-134a","","R-452A","","R-134a","","","R-452A","","","R-452A","","","R-134a","","","R-134a","","","","R-452A","","","R-452A","","","R-134a","","","R-134a","","","R-452A"]
["","GWP","","","","2140","","2140","","1430","","1430","","1430","","1430","","2140","","1430","","","2140","","","2140","","","1430","","","1430","","","","2140","","","2140","","","1430","","","1430","","","2140"]
["Power supply","Voltage","","","V","380-400","","380-400","","220-230","","220-230","","220-230","","220-230","","220-230","","220-230","","","220-230","","","220-230","","","220-230","","","380-400","","","","220-230","","","380-400","","","380-400","","","380-400","","","380-400"]
["","Phase","","","","3N~","","3N~","","1~","","1~","","1~","","1~","","1~","","1~","","","1~","","","1~","","","1~","","","3N~","","","","1~","","","3N~","","","3N~","","","3N~","","","3N~"]
["","Frequency","","","Hz","50","","50","","50","","50","","50","","50","","50","","50","","","50","","","50","","","50","","","50","","","","50","","","50","","","50","","","50","","","50"]
["Dimensions","Evaporator unit","","Height","mm","","215","","280","","215","","215","","215","","215","","215","","215","","","215","","","215","","","215","","","215","","","","215","","","215","","","215","","","215","","","215"]
["","","","Width","mm","","1654","","1530","","654","","654","","654","","654","","654","","654","","","654","","","654","","","1074","","","1074","","","","1074","","","1074","","","1654","","","1654","","","1654"]
["","","","Depth","mm","","410","","690","","410","","410","","410","","410","","410","","410","","","410","","","410","","","410","","","410","","","","410","","","410","","","410","","","410","","","410"]
["Evaporator","Air throw","","","m","","4","","10","","4","","4","","4","","4","","4","","4","","","4","","","4","","","4","","","4","","","","4","","","4","","","4","","","4","","","4"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","","","","0.855","","0.978","","1.12","","1.315","","","","1.351","","","","","","","","","1.806","","","2.034","","","","","","","","","","3.079","","","3.351"]
["Notes","","","","","","","","","","","","","","","","","","","","","","","","","","","(1) - When normally running: 0°C / +30°C","","","(1) - When normally running: 0°C / +30°C","","","(1) - When normally running: 0°C / +30°C","","","","","","","(1) - When normally running: 0°C / +30°C","","","(1) - When normally running: 0°C / +30°C"]
["","","","","","","","","","","","","","","","","","","","","","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]
["","","","","","","","","","","","","","","","","","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","","","(3) - Contains fluorinated greenhouse gases","","","(3) - Contains fluorinated greenhouse gases","","","","","","","(3) - Contains fluorinated greenhouse gases","","","(3) - Contains fluorinated greenhouse gases"]