{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL1"]
[]
[]
[]
[]
["","","","","JEHCCU0115CL1","JEHCCU0135CL1"]
["Weight","Unit","","kg","59","61"]
["Dimensions","Unit","Width","mm","876","876"]
["","","Depth","mm","430","430"]
["","","Height","mm","606","606"]
["Casing","Colour","","","Light grey","Light grey"]
["Fan","Type","","","Axial","Axial"]
["Power supply","Phase","","","1~","1~"]
["","Frequency","","Hz","50","50"]
["","Voltage","","V","230","230"]
["Notes","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room"]
["","","","","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases"]