{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHCCU0180CL3","JEHCCU0210CL3"]
["Refrigerating capacity","Low temperature","R-448A","Nom","kW","0.98"]
["","","R-449A","Nom","kW","0.98"]
["Weight","Unit","","","kg","80","81"]
["Parameters at full load and ambient temp. 25°C","R-448A","Te -35°C","Power input (D2)","kW","1.00"]
["Refrigerant","GWP Type 5","","","","1,387","1,387"]
["","Type 5","","","","R-448A","R-448A"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-448A","Te -10°C","Rated  cooling capacity (PA)","kW","0.98"]
["","","","Rated  power input (DA)","kW","0.98"]
["","R-449A","Te -10°C","Rated  cooling capacity (PA)","kW","0.98"]
["","","","Rated  power input (DA)","kW","0.98"]
["Power input","Low temperature","R-448A","Nom","kW","0.98"]
["","","R-449A","Nom","kW","0.98"]
["Dimensions","Unit","","Width","mm","1,101","1,101"]
["","","","Depth","mm","444","444"]
["","","","Height","mm","662","662"]
["Casing","Colour","","","","Light grey","Light grey"]
["Fan","Type","","","","Axial","Axial"]
["Power supply","Phase","","","","3~","3~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","400","400"]
["Notes","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room"]
["","","","","","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases"]
["COP","Low temperature","","R-448A","","1.00"]
["","","","R-449A","","1.00"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-448A","Te -10°C","Rated COP (COPA)","","1.00"]
["","R-449A","Te -10°C","Rated COP (COPA)","","1.00"]
["Parameters at full load and ambient temp. 25°C","R-448A","Te -35°C","Declared COP (COP2)","","1.15"]
["","R-449A","Te -35°C","Declared COP (COP2)","","1.15"]