{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":19,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CM1"]
[]
[]
[]
[]
["","","","","","JEHCCU0040CM1","JEHCCU0063CM1","JEHCCU0095CM1","JEHCCU0100CM1","JEHCCU0113CM1","JEHCCU0140CM1","JEHCCU0150CM1","JEHCCU0170CM1","JEHCCU0050CM1","JEHCCU0051CM1","JEHCCU0067CM1","JEHCCU0077CM1","JEHCCU0225CM1","JEHCCU0300CM1"]
["Refrigerating capacity","Medium temperature","R-407A","Nom","kW","","","","1.33","1.66","1.92","2.04 (1)","","0.80","","1.07","","3.37 (1)","4.30 (1)"]
["","","R-134a","Nom","kW","0.59","1.06","1.60","","","","1.27 (1)","","","0.89","","1.28","2.06 (1)","2.99 (1)"]
["","","R-404A","Nom","kW","","","","","","","2.27 (1)","","","","","","3.76 (1)","4.81 (1)"]
["","","R-407F","Nom","kW","","","","1.41","1.74","2.08","1.99 (1)","","0.86","","1.15","","3.40 (1)","4.55 (1)"]
["Parameters at full load and ambient temp. 43°C","R-407A","Te -10°C","Declared COP (COP3)","","","","","","","1.56","1.40","","1.42","","","","1.49","1.48"]
["","","","Power input (D3)","kW","","","","","","1.15","1.19","","0.53","","","","1.90","2.49"]
["","","","Cooling capacity (P3)","kW","","","","","","1.79","1.67","","0.76","","","","2.83","3.68"]
["","R-134a","Te -10°C","Power input (D3)","kW","0.36","0.62","0.89","","","","0.85","","","0.53","","0.71","1.21","1.68"]
["","","","Declared COP (COP3)","","1.42","1.40","1.50","","","","1.16","","","1.40","","1.49","1.35","1.49"]
["","","","Cooling capacity (P3)","kW","0.51","0.86","1.34","","","","0.98","","","0.74","","1.06","1.63","2.51"]
["","R-407F","Te -10°C","Declared COP (COP3)","","","","","","","1.58","1.37","","1.46","","","","1.45","1.44"]
["","","","Cooling capacity (P3)","kW","","","","","","1.85","1.74","","0.79","","","","2.86","3.89"]
["","","","Power input (D3)","kW","","","","","","1.17","1.27","","0.54","","","","1.98","2.70"]
["","R-404A","Te -10°C","Power input (D3)","kW","","","","","","","1.34","","","","","","2.14","2.83"]
["","","","Declared COP (COP3)","","","","","","","","1.33","","","","","","1.39","1.36"]
["","","","Cooling capacity (P3)","kW","","","","","","","1.78","","","","","","2.97","3.86"]
["Weight","Unit","","","kg","49","57","58","57","58","67","68","68","49","57","56","58","70","72"]
["Parameters at full load and ambient temp. 25°C","R-407A","Te -10°C","Declared COP (COP2)","","","","","1.74","1.90","1.87","2.00","","1.69","","1.69","","2.09","2.01"]
["","","","Power input (D2)","kW","","","","0.78","0.91","1.04","1.12","","0.48","","0.65","","1.77","2.32"]
["","","","Cooling capacity (P2)","kW","","","","1.35","1.73","1.94","2.25","","0.82","","1.09","","3.69","4.67"]
["","R-407F","Te -10°C","Power input (D2)","kW","","","","0.75","0.89","0.97","1.17","","0.46","","0.62","","1.74","2.43"]
["","","","Cooling capacity (P2)","kW","","","","1.47","1.85","2.15","2.34","","0.89","","1.20","","3.72","5.01"]
["","","","Declared COP (COP2)","","","","","1.95","2.07","2.22","2.00","","1.94","","1.94","","2.14","2.06"]
["","R-404A","Te -10°C","Declared COP (COP2)","","","","","","","","2.01","","","","","","2.11","2.04"]
["","","","Power input (D2)","kW","","","","","","","1.25","","","","","","1.97","2.58"]
["","","","Cooling capacity (P2)","kW","","","","","","","2.51","","","","","","4.15","5.26"]
["","R-134a","Te -10°C","Cooling capacity (P2)","kW","0.62","1.18","1.79","","","","1.41","","","0.97","","1.44","2.26","3.23"]
["","","","Declared COP (COP2)","","1.84","2.05","2.30","","","","1.81","","","2.01","","2.22","2.08","2.15"]
["","","","Power input (D2)","kW","0.34","0.58","0.78","","","","0.78","","","0.48","","0.65","1.09","1.50"]
["Refrigerant","GWP Type 4","","","","","","","","","","1,825.0","","","","","","1,825.0","1,825.0"]
["","GWP Type 5","","","","","","","1,387","1,387","1,387","","1,387","1,387","","1,387"]
["","GWP Type 2","","","","","","","2,107","2,107","2,107","3,921.6","","2,107","","2,107","","3,921.6","3,921.6"]
["","GWP Type 3","","","","","","","1,825","1,825","1,825","2,107.0","","1,825","","1,825","","2,107.0","2,107.0"]
["","GWP","","","","1,430","1,430","1,430","","","","1,430.0","","","1,430","","1,430","1,430.0","1,430.0"]
["","Type 3","","","","","","","R-407F","R-407F","R-407F","R-407A","","R-407F","","R-407F","","R-407A","R-407A"]
["","Type 2","","","","","","","R-407A","R-407A","R-407A","R-404A","","R-407A","","R-407A","","R-404A","R-404A"]
["","Type 5","","","","","","","R-448A","R-448A","R-448A","","R-448A","R-448A","","R-448A"]
["","Type 4","","","","","","","","","","R-407F","","","","","","R-407F","R-407F"]
["","Type","","","","R-134a","R-134a","R-134a","","","","R-134a","","","R-134a","","R-134a","R-134a","R-134a"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-134a","Te -10°C","Rated COP (COPA)","","1.50","1.77","1.86","","","","1.57","","","1.77","","1.85","1.81","1.91"]
["","","","Rated  cooling capacity (PA)","kW","0.59","1.06","1.60","","","","1.27","","","0.89","","1.28","2.06","2.99"]
["","","","Rated  power input (DA)","kW","0.39","0.60","0.86","","","","0.81","","","0.50","","0.70","1.14","1.57"]
["","R-404A","Te -10°C","Rated  power input (DA)","kW","","","","","","","1.28","","","","","","2.03","2.67"]
["","","","Rated  cooling capacity (PA)","kW","","","","","","","2.27","","","","","","3.76","4.81"]
["","","","Rated COP (COPA)","","","","","","","","1.78","","","","","","1.86","1.80"]
["","R-407F","Te -10°C","Rated COP (COPA)","","","","","1.77","1.85","1.93","1.65","","1.77","","1.76","","1.86","1.80"]
["","","","Rated  cooling capacity (PA)","kW","","","","1.41","1.74","2.08","1.99","","0.86","","1.15","","3.40","4.55"]
["","","","Rated  power input (DA)","kW","","","","0.79","0.94","1.07","1.21","","0.49","","0.65","","1.83","2.53"]
["","R-407A","Te -10°C","Rated  power input (DA)","kW","","","","0.80","0.94","1.11","1.15","","0.50","","0.66","","1.82","2.39"]
["","","","Rated COP (COPA)","","","","","1.66","1.78","1.74","1.77","","1.59","","1.62","","1.85","1.80"]
["","","","Rated  cooling capacity (PA)","kW","","","","1.33","1.66","1.92","2.04","","0.80","","1.07","","3.37","4.30"]
["Power input","Medium temperature","R-134a","Nom","kW","0.39","0.60","0.86","","","","0.810 (1)","","","0.50","","0.70","1.140 (1)","1.570 (1)"]
["","","R-404A","Nom","kW","","","","","","","1.280 (1)","","","","","","2.030 (1)","2.670 (1)"]
["","","R-407F","Nom","kW","","","","0.79","0.94","1.07","1.210 (1)","","0.49","","0.65","","1.830 (1)","2.530 (1)"]
["","","R-407A","Nom","kW","","","","0.80","0.94","1.11","1.150 (1)","","0.50","","0.66","","1.820 (1)","2.390 (1)"]
["COP","Medium temperature","","R-134a","","1.50","1.77","1.86","","","","1.57 (1)","","","1.77","","1.85","1.81 (1)","1.91 (1)"]
["","","","R-407F","","","","","1.77","1.85","1.93","1.65 (1)","","1.77","","1.76","","1.86 (1)","1.80 (1)"]
["","","","R-407A","","","","","1.66","1.78","1.74","1.77 (1)","","1.59","","1.62","","1.85 (1)","1.80 (1)"]
["","","","R-404A","","","","","","","","1.78 (1)","","","","","","1.86 (1)","1.80 (1)"]
["Dimensions","Unit","","Width","mm","876","876","876","876","876","1,101","1,101","1,101","876","876","876","876","1,101","1,101"]
["","","","Depth","mm","430","430","430","430","430","444","444","444","430","430","430","430","444","444"]
["","","","Height","mm","606","606","606","606","606","662","662","662","606","606","606","606","662","662"]
["Casing","Colour","","","","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey"]
["Fan","Type","","","","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","230","230","230","230","230","230","230","230","230"]
["Notes","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - Refer to condition: Outside ambient temperature = 32°C, Evaporation temperature = -10°C and 10K superheat (medium temperature application)","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - Refer to condition: Outside ambient temperature = 32°C, Evaporation temperature = -10°C and 10K superheat (medium temperature application)","(1) - Refer to condition: Outside ambient temperature = 32°C, Evaporation temperature = -10°C and 10K superheat (medium temperature application)"]
["","","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room"]
["","","","","","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases"]
["","","","","","","","","","","","(4) - Contains fluorinated greenhouse gases","","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]