{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":8,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CM1"]
[]
[]
[]
[]
["","","","","","JEHSCU0200CM1","JEHSCU0250CM1","JEHSCU0300CM1"]
["Refrigerating capacity","Medium temperature","R-407A","Nom","kW","3.48","4.09"]
["","","R-134a","Nom","kW","2.13"]
["","","R-407F","Nom","kW","3.33","3.82","4.63"]
["Parameters at full load and ambient temp. 43°C","R-134a","Te -10°C","Power input (D3)","kW","1.32"]
["","","","Declared COP (COP3)","","1.42"]
["","","","Cooling capacity (P3)","kW","1.87"]
["Weight","Unit","","","kg","69.7","71.7","73.7"]
["Parameters at full load and ambient temp. 25°C","R-407A","Te -10°C","Declared COP (COP2)","","2.61","2.44"]
["","","","Power input (D2)","kW","1.42","1.78"]
["","","","Cooling capacity (P2)","kW","3.72","4.35"]
["","R-407F","Te -10°C","Power input (D2)","kW","1.50","1.82","2.30"]
["","","","Cooling capacity (P2)","kW","3.68","4.26","5.09"]
["","","","Declared COP (COP2)","","2.46","2.33","2.21"]
["","R-134a","Te -10°C","Cooling capacity (P2)","kW","2.25"]
["","","","Declared COP (COP2)","","2.21"]
["","","","Power input (D2)","kW","1.02"]
["Refrigerant","GWP Type 5","","","","1,387","1,387","1,387"]
["","GWP Type 2","","","","2,107","2,107"]
["","GWP Type 3","","","","1,825","1,825","1,825"]
["","GWP","","","","1,430"]
["","Type 3","","","","R-407F","R-407F","R-407F"]
["","Type 2","","","","R-407A","R-407A"]
["","Type 5","","","","R-448A","R-448A","R-448A"]
["","Type","","","","R-134a"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-134a","Te -10°C","Rated COP (COPA)","","1.92"]
["","","","Rated  cooling capacity (PA)","kW","2.13"]
["","","","Rated  power input (DA)","kW","1.11"]
["","R-407F","Te -10°C","Rated COP (COPA)","","1.92","1.83","1.74"]
["","","","Rated  cooling capacity (PA)","kW","3.33","3.82","4.63"]
["","","","Rated  power input (DA)","kW","1.74","2.09","2.66"]
["","R-407A","Te -10°C","Rated  power input (DA)","kW","1.60","1.98"]
["","","","Rated COP (COPA)","","2.18","2.06"]
["","","","Rated  cooling capacity (PA)","kW","3.48","4.09"]
["Power input","Medium temperature","R-134a","Nom","kW","1.11"]
["","","R-407F","Nom","kW","1.74","2.09","2.66"]
["","","R-407A","Nom","kW","1.60","1.98"]
["COP","Medium temperature","","R-134a","","1.92"]
["","","","R-407F","","1.92","1.83","1.74"]
["","","","R-407A","","2.18","2.06"]
["Dimensions","Unit","","Width","mm","1,101","1,101","1,101"]
["","","","Depth","mm","444","444","444"]
["","","","Height","mm","662","662","662"]
["Casing","Colour","","","","Light grey","Light grey","Light grey"]
["Fan","Type","","","","Axial","Axial","Axial"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Notes","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room"]
["","","","","","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases"]