{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":66,"n_cols":16,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CM3"]
[]
[]
[]
[]
["","","","","","JEHSCU0360CM3","JEHSCU0800CM3","JEHSCU1000CM3","JEHSCU0200CM3","JEHSCU0250CM3","JEHSCU0300CM3","JEHSCU0350CM3","JEHSCU0400CM3","JEHSCU0500CM3","JEHSCU0600CM3","JEHSCU0680CM3"]
["Refrigerating capacity","Medium temperature","R-407A","Nom","kW","5.77","12.95","","3.45","4.05","4.69","","6.76","8.28","9.54","10.70"]
["","","R-134a","Nom","kW","3.80","8.21","10.75","2.24","","","3.48","4.37"]
["","","R-407F","Nom","kW","5.73","12.90","","3.33","3.94","4.58","","6.75","8.18","9.59"]
["Annual electricity consumption Q","R-407A","","Te -10°C","kWh/a","10,186.80","25,490.84","","","","","","10,972.69","15,847.87","18,407.87","22,239.63"]
["","R-134a","","Te -10°C","kWh/a","","16,256.53","19,586.43"]
["","R-407F","","Te -10°C","kWh/a","10,932.85","26,882.45","","","","","","11,873.19","16,401.48","18,902.83"]
["Parameters at full load and ambient temp. 43°C","R-134a","Te -10°C","Power input (D3)","kW","","4.56","5.92","","","","2.02"]
["","","","Declared COP (COP3)","","","1.59","1.60","","","","1.52"]
["","","","Cooling capacity (P3)","kW","","7.26","9.46","","","","3.06"]
["Weight","Unit","","","kg","112","204","226","69.7","71.7","73.7","73.7","119","123","125","126"]
["Parameters at full load and ambient temp. 25°C","R-407A","Te -10°C","Declared COP (COP2)","","","","","2.55","2.36","2.26"]
["","","","Power input (D2)","kW","","","","1.44","1.82","2.22"]
["","","","Cooling capacity (P2)","kW","","","","3.69","4.31","5.00"]
["","R-407F","Te -10°C","Power input (D2)","kW","","","","1.52","1.88","2.36"]
["","","","Cooling capacity (P2)","kW","","","","3.64","4.31","5.06"]
["","","","Declared COP (COP2)","","","","","2.39","2.29","2.14"]
["","R-134a","Te -10°C","Cooling capacity (P2)","kW","4.06","","","2.38","","","3.71","4.70"]
["","","","Declared COP (COP2)","","2.86","","","2.62","","","2.46","2.90"]
["","","","Power input (D2)","kW","1.42","","","0.91","","","1.51","1.62"]
["Seasonal energy performance ratio SEPR","R-407F","","Te -10°C","","3.22","2.95","","","","","","3.50","3.07","3.12"]
["","R-407A","","Te -10°C","","3.48","3.12","","","","","","3.79","3.21","3.19","2.96"]
["","R-134a","","Te -10°C","","","3.10","3.37"]
["Refrigerant","GWP Type 4","","","","1,495","1,495","","1,495","1,495","1,495","","1,495","","1,495","1,495"]
["","GWP Type 5","","","","1,387","1,387","1,387","1,387","1,387","1,387","1,387","1,387","1,387","1,387","1,387"]
["","GWP Type 2","","","","2,107","2,107","","2,107","2,107","2,107","","2,107","2,107","2,107","2,107"]
["","GWP Type 3","","","","1,825","1,825","","1,825","1,825","1,825","","1,825","1,825","1,825"]
["","GWP","","","","1,430","1,430","1,430","1,430","","","1,430","1,430"]
["","Type 3","","","","R-407F","R-407F","","R-407F","R-407F","R-407F","","R-407F","R-407F","R-407F"]
["","Type 2","","","","R-407A","R-407A","","R-407A","R-407A","R-407A","","R-407A","R-407A","R-407A","R-407A"]
["","Type 5","","","","R-448A","R-448A","R-448A","R-448A","R-448A","R-448A","R-448A","R-448A","R-448A","R-448A","R-448A"]
["","Type 4","","","","R-407H","R-407H","","R-407H","R-407H","R-407H","","R-407H","","R-407H","R-407H"]
["","Type","","","","R-134a","R-134a","R-134a","R-134a","","","R-134a","R-134a"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-134a","Te -10°C","Rated COP (COPA)","","2.36","2.20","2.21","2.18","","","2.08","2.36"]
["","","","Rated  cooling capacity (PA)","kW","3.80","8.21","10.75","2.24","","","3.48","4.37"]
["","","","Rated  power input (DA)","kW","1.61","3.74","4.86","1.02","","","1.68","1.85"]
["","R-407F","Te -10°C","Rated COP (COPA)","","1.97","2.10","","1.88","1.83","1.69","","2.10","1.88","1.91"]
["","","","Rated  cooling capacity (PA)","kW","5.73","12.90","","3.33","3.94","4.58","","6.75","8.18","9.59"]
["","","","Rated  power input (DA)","kW","2.91","6.13","","1.78","2.16","2.70","","3.21","4.36","5.03"]
["","R-407A","Te -10°C","Rated  power input (DA)","kW","2.58","6.24","","1.62","2.04","2.44","","2.97","3.93","4.65","5.54"]
["","","","Rated COP (COPA)","","2.24","2.08","","2.12","1.99","1.92","","2.28","2.11","2.05","1.93"]
["","","","Rated  cooling capacity (PA)","kW","5.77","12.95","","3.45","4.05","4.69","","6.76","8.28","9.54","10.70"]
["Power input","Medium temperature","R-134a","Nom","kW","1.61","3.74","4.86","1.02","","","1.68","1.85"]
["","","R-407F","Nom","kW","2.91","6.13","","1.78","2.16","2.70","","3.21","4.36","5.03"]
["","","R-407A","Nom","kW","2.58","6.24","","1.62","2.04","2.44","","2.97","3.93","4.65","5.54"]
["COP","Medium temperature","","R-134a","","2.36","2.20","2.21","2.18","","","2.08","2.36"]
["","","","R-407F","","1.97","2.10","","1.88","1.83","1.69","","2.10","1.88","1.91"]
["","","","R-407A","","2.24","2.08","","2.12","1.99","1.92","","2.28","2.11","2.05","1.93"]
["Dimensions","Unit","","Width","mm","1,353","1,348","1,348","1,101","1,101","1,101","1,101","1,353","1,353","1,353","1,353"]
["","","","Depth","mm","575","612","612","444","444","444","444","575","575","575","575"]
["","","","Height","mm","872","1,727","1,727","662","662","662","662","872","872","872","872"]
["Casing","Colour","","","","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey"]
["Fan","Type","","","","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial","Axial"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","400","400","400","400","400","400","400","400","400","400","400"]
["Notes","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - Refer to condition: Outside ambient temperature = 32°C, Evaporation temperature = -10°C and 10K superheat (medium temperature application)","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room"]
["","","","","","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases"]
["","","","","","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H","","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H","","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H","","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H","(4) - Published data based on condition - Return Gas Temperature 20°C, except for R-407H"]
["","","","","","(5) - Published data based on condition - SH10K for R-407H","(5) - Published data based on condition - SH10K for R-407H","","(5) - Published data based on condition - SH10K for R-407H","(5) - Published data based on condition - SH10K for R-407H","(5) - Published data based on condition - SH10K for R-407H","","(5) - Published data based on condition - SH10K for R-407H","","(5) - Published data based on condition - SH10K for R-407H","(5) - Published data based on condition - SH10K for R-407H"]