{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEN-AY1"]
[]
[]
[]
[]
["","","","","","LRYEN10A7Y1"]
["Casing","Colour","","","","Ivory white"]
["Dimensions","Unit","","Height","mm","1680"]
["","","","Width","mm","1930"]
["","","","Depth","mm","765"]
["Weight","Unit","","","kg","563"]
["Fan","Type","","","","Propeller fan"]
["","Quantity","","","","3"]
["","Air flow rate","Cooling","Nom.","m³/min","300"]
["Fan motor","Output","","","W","750"]
["Heat exchanger","Type","","","","Cross fin coil"]
["Refrigerant","Type 2","","","","R-744"]
["","GWP","","","","1.0"]
["","Charge","","","kg","6.30"]
["Standard Accessories","Installation manual","","","","1"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Copper packing for stop valve (15 pcs)","","","","1"]
["","Copper packing for service port (15 pcs)","","","","1"]
["","Declaration of conformity","","","","1"]
["Power supply","Phase","","","","3N~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Notes","","","","","(1) - Compressor 1"]
["","","","","","(2) - Compressor 2"]
["","","","","","(3) - Compressor 3"]
["","","","","","(4) - Factory charge of unit"]