{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Type","","","","","Humidifying air purifier"]
["Application","","","","","Floor standing type"]
["Casing","Colour","","","","White"]
["Dimensions","Unit","","Height","mm","700"]
["","","","Width","mm","270"]
["","","","Depth","mm","270"]
["Weight","Unit","","","kg","9.5"]
["Applicable room area","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Air purifying operation","Power input","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Silent","kW","0.007"]
["Humidifying operation","Power input","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Silent","kW","0.011"]
["","Water tank capacity","","","l","2.7"]
["Sound pressure level","Air purifying operation","","Turbo","dBA","53.0"]
["","","","Medium","dBA","39.0"]
["","","","Low","dBA","29.0"]
["","","","Silent","dBA","19.0"]
["","Humidifying operation","","Turbo","dBA","53.0"]
["","","","Medium","dBA","39.0"]
["","","","Low","dBA","33.0"]
["","","","Silent","dBA","25.0"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","330"]
["","","","Medium","m³/h","192"]
["","","","Low","m³/h","120"]
["","","","Silent","m³/h","54"]
["","","Humidifying operation","Turbo","m³/h","330"]
["","","","Medium","m³/h","192"]
["","","","Low","m³/h","144"]
["","","","Silent","m³/h","102"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Flash streamer + Deodorizing catalyst"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Power cord","Power cord","","","","1.8"]
["Power supply","Phase","","","","1~"]
["","Power supply-=-Frequency","","Frequency","","50/60"]
["","Power supply-=-Voltage","","Voltage","","220-240/220-230"]
["Running current","Air purifying operation","Running current-=-Air purifying operation-=-Turbo","Turbo","","0.50"]
["","","Running current-=-Air purifying operation-=-Medium","Medium","","0.19"]
["","","Running current-=-Air purifying operation-=-Low","Low","","0.12"]
["","","Running current-=-Air purifying operation-=-Silent","Silent","","0.09"]
["","Humidifying operation","Running current-=-Humidifying operation-=-Turbo","Turbo","","0.50"]
["","","Running current-=-Humidifying operation-=-Medium","Medium","","0.20"]
["","","Running current-=-Humidifying operation-=-Low","Low","","0.15"]
["","","Running current-=-Humidifying operation-=-Silent","Silent","","0.13"]
["Notes","","","","","(1) - The applicable room area is appropriate for operating the unit of maximum fan speed (HH). Applicable room area indicates  the space where a certain amount of dust particles can be remover in 30 minutes. (JEM 1467)"]
["","","","","","(2) - Converted to NRCC standards from test values in accordance with JEM1467."]