{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":14,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","R2TND-A4A"]
[]
[]
[]
[]
["","","","","","R2TND012A4AA","R2TND012A4AB","R2TND018A4AA","R2TND018A4AB","R2TND024A4AA","R2TND024A4AB","R2TND028A4AA","R2TND028A4AB","R2TND035A4AB"]
["Heat losses","Stand-by boiler Ps","","","kW","","","","","","","","","0.065"]
["Domestic hot water","Heat input (gross calorific value) Qnw","Nom","Max","kW","","","","","","","","","37.7"]
["","","","Min","kW","","","","","","","","","5.3"]
["","Temperature","","Max","°C","","","","","","","","","60"]
["","Heat input (net calorific value) Qnw","Nom","Min","kW","","","","","","","","","4.8"]
["","","","Max","kW","","","","","","","","","34"]
["Flue gas","Mass flow (G25)","","Max","kg/h","","","","","","","","","49.6"]
["","Mass flow (G20)","","Max","kg/h","","","","","","","","","55.7"]
["","Mass flow (G31)","","Max","kg/h","","","","","","","","","54.7"]
["","Temperature","","Max","°C","","","","","","","","","81.7"]
["Supply air","Concentric","","","","","","","","","","","","Yes"]
["Dimensions","Unit","Height","Casing","mm","","","","","","","","","690"]
["Casing","Material","","","","","","","","","","","","Powder painted galvanised steel plate"]
["","Colour","","","","","","","","","","","","Titanium White (Ral9003)"]
["Space heating","General","","ηs (Seasonal space heating efficiency)","%","","","","","","","","","93"]
["","","","Seasonal space heating eff. class","","","","","","","","","","A"]
["Central heating","Heat input Qn (gross calorific value)","Nom","Min","kW","","","","","","","","","5.3"]
["","","","Max","kW","","","","","","","","","37.8"]
["","Water temperature","","Max","°C","","","","","","","","","100"]
["","Output at 37/30°C","","Nom","kW","","","","","","","","","11.1"]
["","Output Pn at 80/60°C","","Min","kW","","","","","","","","","4.6"]
["","","","Nom","kW","","","","","","","","","33.2"]
["","Heat input Qn (net calorific value)","Nom","Min","kW","","","","","","","","","4.8"]
["","","","Max","kW","","","","","","","","","34"]
["","Output Pnc at 50/30°C","","Min","kW","","","","","","","","","5.2"]
["","","","Nom","kW","","","","","","","","","35"]
["Gas","NOx level (G20)","","","mg/kWh","","","","","","","","","35.5"]
["","Consumption (G25)","","Min","m³/h","","","","","","","","","0.59"]
["","","","Max","m³/h","","","","","","","","","4.19"]
["","NOx class","","","","","","","","","","","","6"]
["","Consumption (G20)","","Max","m³/h","","","","","","","","","3.63"]
["","","","Min","m³/h","","","","","","","","","0.511"]
["","Consumption (G31)","","Min","m³/h","","","","","","","","","0.2"]
["","","","Max","m³/h","","","","","","","","","1.38"]
["","Consumption (G20)","","Min","m³/h","0.31","0.31","0.31","0.31","0.31","0.31","0.511","0.511"]
["","","","Max","m³/h","1.18","1.18","1.80","1.8","2.48","2.48","2.89","2.89"]
["","Consumption (G25)","","Min","m³/h","0.36","0.36","0.36","0.36","0.36","0.36","0.59","0.59"]
["","","","Max","m³/h","1.38","1.38","2.09","2.09","2.89","2.89","3.32","3.32"]
["","Consumption (G31)","","Min","m³/h","0.12","0.12","0.12","0.12","0.12","0.12","0.2","0.2"]
["","","","Max","m³/h","0.46","0.46","0.69","0.69","0.96","0.96","1.1","1.1"]
["","NOx class","","","","6","6","6","6","6","6","6","6"]
["","","","","","10","10","18","18","22","22","36.3","36"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","2.9","2.9","2.9","2.9","2.9","2.9","4.8","4.8"]
["","","","Max","kW","11.2","11.1","17.0","16.9","23.5","23.5","27","27"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","3.2","3.2","3.2","3.2","3.2","3.2","5.3","5.3"]
["","","","Max","kW","12.4","12.3","18.9","18.8","26.1","26.1","30","30"]
["","Output Pn at 80/60°C","","Min","kW","2.8","2.8","2.8","2.8","2.8","2.8","4.6","4.6"]
["","","","Nom","kW","10.9","10.9","16.6","16.6","22.8","22.8","26.3","26.3"]
["","Output Pnc at 50/30°C","","Min","kW","3.1","3.1","3.1","3.1","3.1","3.1","5.2","5.2"]
["","","","Nom","kW","12.0","12","18.0","18","24.0","24","28.2","28.2"]
["","Output at 37/30°C","","Nom","kW","3.7","3.7","5.6","5.5","7.6","7.6","8.8","8.8"]
["","Water temperature","","Max","°C","100","100","100","100","100","100","100","100"]
["","Efficiency","","Net calorific value","%","98.6","98.6","98.2","98.18","97.9","97.9"]
["","","","Gross calorific value","%","87.8","87.8","87.4","87.4","87.3","87.3"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","2.9","2.9","2.9","2.9","2.9","2.9","4.8","4.8"]
["","","","Max","kW","11.2","11.1","17.0","16.9","23.5","23.5","29.5","29.5"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","3.2","3.2","3.2","3.2","3.2","3.2","5.3","5.3"]
["","","","Max","kW","12.4","12.3","18.1","18.1","26.1","26.1","32.7","32.7"]
["","Temperature","","Max","°C","60","60","60","60","60","60","60","60"]
["Heat losses","Stand-by boiler Ps","","","kW","0.057","0.057","0.057","0.057","0.057","0.057","0.0650","0.065"]
["Supply air","Connection","","","mm","100","100","100","100","100","100","100","100"]
["","Concentric","","","","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes"]
["Flue gas","Temperature","","Max","°C","90","90","90","90","90","90","76.4","76.4"]
["","Connection","","","mm","60","60","60","60","60","60","60","60"]
["","Mass flow (G20)","","Max","kg/h","38.7","38.7","38.7","38.7","38.7","38.7","44.5","55.7"]
["","Mass flow (G31)","","Max","kg/h","36.0","36","36.0","36","36.0","36","43.3","43.3"]
["Casing","Colour","","","","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)"]
["","Material","","","","Sheet metal","Sheet metal","Sheet metal","Sheet metal","Sheet metal","Sheet metal","Powder painted galvanised steel plate","Powder painted galvanised steel plate"]
["Dimensions","Unit","Height","Casing","mm","590","590","590","590","590","590","690","690"]
["","","","Width","mm","400","400","400","400","400","400","440","440"]
["","","","Depth","mm","256","256","256","256","256","256","295","295"]
["Weight","Unit","","Empty","kg","27","1","27","1","27","1","35.5","1"]
["","","","Full","kg","27","26.5","27","26.5","27","26.5","37.5"]
["","Boiler","","Empty","kg","26.5","26.5","26.5","26.5","26.5","26.5"]
["Space heating","General","","Seasonal space heating eff. class","","A","A","A","A","A","A","A","A"]
["Flue gas","Mass flow (G25)","","Max","kg/h","","","","","","","39.3","39.3"]