{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":21,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RCV"]
[]
[]
[]
[]
["","","","","","RCV101001E","RCV101002E","RCV101527E","RCV101528E","RCV102001E","RCV102002E","RCV102528E","RCV102527E","RCV201001E","RCV201002E","RCV201527E","RCV201528E","RCV202002E","RCV202527E","RCV202528E","RCV202001E"]
["Refrigerant","GWP","","","","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430"]
["","Type","","","","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a"]
["Refrigerating capacity","High temperature","R-134a","Nom","kW","0.6","0.6","0.6","0.6","1","1","1","1","1.4","1.4","1.4","1.4","2.3","2.3","2.3","2.3"]
["Dimensions","Unit","","Width","mm","400","400","400","400","400","400","400","400","620","620","620","620","620","620","620","620"]
["","","","Depth","mm","435","435","435","435","435","435","435","435","435","435","435","435","435","435","435","435"]
["","","","Height","mm","735","735","735","735","735","735","735","735","735","735","735","735","735","735","735","735"]
["Compressor","Nominal power","","","kW","0.25","0.25","0.25","0.25","0.37","0.37","0.37","0.37","0.46","0.46","0.46","0.46","0.55","0.55","0.55","0.55"]
["","Type","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating"]
["Weight","Unit","","","kg","49","50","49","50","52","53","53","52","77","78","77","78","80","79","80","79"]
["Heating capacity","R-134a","","Nom","kW","0.7","0.7","0.7","0.7","1.05","1.05","1.05","1.05","1.4","1.4","1.4","1.4","1.75","1.75","1.75","1.75"]
["Evaporator","Air throw","","","m","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230"]
["Notes","","","","","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C"]
["","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]
["","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]