{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":53,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RDV"]
[]
[]
[]
[]
["","","","","","SB.RDV101523E","SB.RDV101524E","SB.RDV101525E","SB.RDV101529E","SB.RDV102523E","SB.RDV102524E","SB.RDV102525E","SB.RDV102529E","SB.RDV201523E","SB.RDV201524E","SB.RDV201525E","SB.RDV201529E","SB.RDV202523E","SB.RDV202524E","SB.RDV202525E","SB.RDV202529E","SB.RDV101001E","SB.RDV101002E","SB.RDV101021E","SB.RDV101022E","SB.RDV102001E","SB.RDV102002E","SB.RDV102021E","SB.RDV102022E","RDV103EA12S3A","RDV103EA12S3B","RDV103EA12S7A","RDV103EA12S7B","RDV105EA12S3A","RDV105EA12S3B","RDV105EA12S7A","RDV105EA12S7B","SB.RDV201001E","SB.RDV201002E","SB.RDV201021E","SB.RDV201022E","SB.RDV202001E","SB.RDV202002E","SB.RDV202021E","SB.RDV202022E","RDV206EA12S3A","RDV206EA12S3B","RDV206EA12S7A","RDV206EA12S7B","RDV207EA12S3A","RDV207EA12S3B","RDV207EA12S7A","RDV207EA12S7B"]
["Refrigerant","GWP","","","","","","","","","","","","","","","","","","","","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430","","","","","","","","","1,430","1,430","1,430","1,430","1,430","1,430","1,430","1,430"]
["","Type","","","","","","","","","","","","","","","","","","","","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","","","","","","","","","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a"]
["Refrigerating capacity","High temperature","R-134a","Nom","kW","","","","","","","","","","","","","","","","","0.600 (1)","0.600 (1)","0.600 (1)","0.600 (1)","1.000 (1)","1.000 (1)","1.000 (1)","1.000 (1)","","","","","","","","","1.400 (1)","1.400 (1)","1.400 (1)","1.400 (1)","2.300 (1)","2.300 (1)","2.300 (1)","2.300 (1)"]
["Standard liquid receiver","l","","","","","","","","","","","","","","","","","","","","1.6","1.6","1.6","1.6","1.6","1.6","1.6","1.6","1.6","","1.6","","2.5","","2.5","","2.5","2.5","2.5","2.5","2.5","2.5","2.5","2.5","1.6","","1.6","","2.5","","2.5"]
["Dimensions","Evaporator unit","","Depth","mm","","","","","","","","","","","","","","","","","210","210","490","490","210","210","490","490","","","","","","","","","210","210","490","490","210","210","490","490"]
["","","","Height","mm","","","","","","","","","","","","","","","","","570","570","215","215","570","570","215","215","","","","","","","","","570","570","215","215","570","570","215","215"]
["","","","Width","mm","","","","","","","","","","","","","","","","","375","375","669","669","375","375","669","669","","","","","","","","","595","595","1,089","1,089","595","595","195","1,089"]
["","Condensing unit","","Depth","mm","","","","","","","","","","","","","","","","","337","337","337","337","337","337","337","337","","","","","","","","","427","427","427","427","427","427","427","427"]
["","","","Width","mm","","","","","","","","","","","","","","","","","682","682","682","682","682","682","682","682","","","","","","","","","882","882","882","882","882","882","882","882"]
["Compressor","Nominal power","","","kW","","","","","","","","","","","","","","","","","0.25","0.25","0.25","0.25","0.37","0.37","0.37","0.37","","","","","","","","","0.46","0.46","0.46","0.46","0.55","0.55","0.55","0.55"]
["","Type","","","","","","","","","","","","","","","","","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","","","","","","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating"]
["","Starting method","","","","","","","","","","","","","","","","","","","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","","","","","","","","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct"]
["Heating capacity","R-134a","","Nom","kW","","","","","","","","","","","","","","","","","0.700","0.700","0.900","0.900","1.050","1.050","0.900","0.900","","","","","","","","","1.400","1.400","1.600","1.600","1.750 (1)","1.750 (1)","1.600","1.600"]
["Evaporator","Air throw","","","m","","","","","","","","","","","","","","","","","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","","","","","","","","","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)"]
["Power supply","Phase","","","","","","","","","","","","","","","","","","","","1~","1~","1~","1~","1~","1~","1~","1~","","","","","","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","","","","","","","","","","","","","","","","","50","50","50","50","50","50","50","50","","","","","","","","","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","","","","","","","","","","","","","","","","","230","230","230","230","230","230","230","230","","","","","","","","","230","230","230","230","230","230","230","230"]
["Notes","","","","","","","","","","","","","","","","","","","","","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","","","","","","","","","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C","(1) - When normally running: +10°C / +30°C"]
["","","","","","","","","","","","","","","","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]
["","","","","","","","","","","","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]
["Refrigerating capacity","High temperature","R-134a","Nom","kW","0.6","0.6","0.6","0.6","1","1","1","1","1.4","1.4","1.4","1.4","2.3","2.3","2.3","2.3"]
["Heating capacity","R-134a","","Nom","kW","0.7","0.9","0.9","0.7","1.05","0.9","0.9","1.05","1.4","1.6","1.6","1.4","1.75","1.6","1.6","1.75","","","","","","","","","","0.7","","0.9","","1.05","","0.9","","","","","","","","","","1.4","","1.6","","1.75","","1.6"]
["Dimensions","Condensing unit","","Width","mm","682","682","682","682","682","682","682","682","882","882","882","882","882","882","882","882","","","","","","","","","682","","682","","682","","682","","","","","","","","","","882","","882","","882","","882"]
["","","","Depth","mm","337","337","337","337","337","337","337","337","427","427","427","427","427","427","427","427","","","","","","","","","337","","337","","337","","337","","","","","","","","","","427","","427","","427","","427"]
["","Evaporator unit","","Height","mm","570","215","215","570","570","215","215","570","570","215","215","570","570","215","215","570","","","","","","","","","","570","","215","","570","","215","","","","","","","","","","570","","215","","570","","215"]
["","","","Width","mm","375","669","669","375","375","669","669","375","595","1089","1089","595","595","195","1089","595","","","","","","","","","","375","","669","","375","","669","","","","","","","","","","595","","1089","","595","","1089"]
["","","","Depth","mm","210","490","490","210","210","490","490","210","210","490","490","210","210","490","490","210","","","","","","","","","","210","","490","","210","","490","","","","","","","","","","210","","490","","210","","490"]
["Compressor","Type","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","","","","","","","","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","","","","","","","","","Hermetic","","Hermetic","","Hermetic","","Hermetic"]
["","Starting method","","","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","","","","","","","","","Direct","","Direct","","Direct","","Direct","","","","","","","","","","Direct","","Direct","","Direct","","Direct"]
["Condenser","Air flow","","","m³/h","600","600","600","600","600","600","600","600","1200","1100","1100","1200","1200","1100","1100","1200","","","","","","","","","600","","600","","1200","","1200","","","","","","","","","","600","","600","","1100","","1100"]
["Refrigerant","Type","","","","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","","","","","","","","","R-134a","","R-134a","","R-134a","","R-134a","","","","","","","","","","R-134a","","R-134a","","R-134a","","R-134a"]
["Power supply","Voltage","","","V","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","","","","","","","","","220-230","","220-230","","220-230","","220-230","","","","","","","","","","220-230","","220-230","","220-230","","220-230"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","","","","","","","","","1~","","1~","","1~","","1~","","","","","","","","","","1~","","1~","","1~","","1~"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","","","","","","","","","","","","","","","","","","","","","","","","0.593","","0.593","","0.912","","0.912","","","","","","","","","","1.336","","1.336","","1.935","","1.935"]
["Casing","Colour","","Condensing unit","","","","","","","","","","","","","","","","","","","","","","","","","","Purple","Purple","Purple","Purple","Purple","Purple","Purple","Purple","","","","","","","","","Purple","Purple","Purple","Purple","Purple","Purple","Purple","Purple"]
["Compressor","Quantity","","","","","","","","","","","","","","","","","","","","","","","","","","","","1","","1","","1","","1","","","","","","","","","","1","","1","","1","","1"]
["","Model","","","","","","","","","","","","","","","","","","","","","","","","","","","","AE4430Y-FZ1A","","AE4430Y-FZ1A/CSIR","","NEU6212Z/CSI","","NEU6212Z/CSIR","","","","","","","","","","CAJ4476Y/F/CSIR","","CAJ4476Y/F/CSIR","","CAJ4511Y/F","","CAJ4511Y/F"]
["Evaporator","Air throw","","","m","","","","","","","","","","","","","","","","","","","","","","","","","4","","4","","4","","4","","","","","","","","","","4","","4","","4","","4"]
["Operation range","Cold room temperature","","Min.","°C","","","","","","","","","","","","","","","","","","","","","","","","","10","","10","","10","","10","","","","","","","","","","10","","10","","10","","10"]
["","","","Max.","°C","","","","","","","","","","","","","","","","","","","","","","","","","20","","20","","20","","20","","","","","","","","","","20","","20","","20","","20"]
["","Ambient temperature","","Min.","°C","","","","","","","","","","","","","","","","","","","","","","","","","20","","20","","20","","20","","","","","","","","","","20","","20","","20","","20"]
["","","","Max.","°C","","","","","","","","","","","","","","","","","","","","","","","","","40","","40","","40","","40","","","","","","","","","","40","","40","","40","","40"]
["Refrigerant","GWP","","","","","","","","","","","","","","","","","","","","","","","","","","","","1430","","1430","","1430","","1430","","","","","","","","","","1430","","1430","","1430","","1430"]
["Sound pressure level","Nom.","","","dBA","","","","","","","","","","","","","","","","","","","","","","","","","35","","35","","35","","35","","","","","","","","","","43","","43","","43","","43"]
["Power supply","Frequency","","","Hz","","","","","","","","","","","","","","","","","","","","","","","","","50","","50","","50","","50","","","","","","","","","","50","","50","","50","","50"]