{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":5,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RDXYQ-TA"]
[]
[]
[]
[]
["","","","","RDXYQ5TAV1B"]
["Sound pressure level","Cooling","Nom.","dBA","54 (5)"]
["Standard Accessories","Installation and operation manual","","","1"]
["","Drain hose","","","1"]
["","Screws","","","1"]
["","Tie-wraps","","","1"]
["","Hose band","","","1"]
["Weight","Unit","","kg","103"]
["Refrigerant","Type","","","R-410A"]
["Piping connections","Drain","OD","mm","32"]
["Sound power level","Cooling","Nom.","dBA","81 (4)"]
["Dimensions","Unit","Width","mm","1,456"]
["","","Depth","mm","1,044"]
["","","Height","mm","397"]
["","Ducting","Height","mm","298"]
["","","Width","mm","1,196"]
["Power supply","Phase","","","1N~"]
["","Name","","","V1"]
["","Frequency","","Hz","50"]
["","Voltage","","V","220-240"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","(3) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%)."]
["","","","","(4) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","(5) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to sound level drawings. Nominal air flow rate, ESP 60 Pa."]
["","","","","(6) - Refer to refrigerant pipe selection or installation manual"]
["","","","","(7) - In accordance with EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply wih Ssc  ≥ minimum Ssc value"]
["","","","","(8) - Sound values are measured in a semi-anechoic room."]
["","","","","(9) - Contains fluorinated greenhouse gases"]