{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RHSX-D / RRGA04-08DV"]
[]
[]
[]
[]
["","","","","RHSX04P30DA / RRGA04DAV3","RHSX04P50DA / RRGA04DAV3","RHSX08P30DA / RRGA06DAV3","RHSX08P50DA / RRGA06DAV3","RHSX08P30DA / RRGA08DAV3","RHSX08P50DA / RRGA08DAV3"]
["Domestic hot water heating","General","Declared load profile","","L","XL","L","XL","L","XL"]
["","Average climate","Water heating energy efficiency class","","A","A","A","A","A","A"]
["COP","","","","4.93 (1), 3.54 (2)","4.93 (1), 3.54 (2)","4.95 (1), 3.50 (2)","4.95 (1), 3.50 (2)","4.48 (1), 3.49 (2)","4.48 (1), 3.49 (2)"]
["Indoor unit","","","","RHSX04P30D","RHSX04P50D","RHSX08P30D","RHSX08P50D","RHSX08P30D","RHSX08P50D"]
["Cooling capacity","Nom.","","kW","5.06 (1), 4.46 (2)","5.06 (1), 4.46 (2)","6.19 (1), 4.96 (2)","6.19 (1), 4.96 (2)","6.44 (1), 5.46 (2)","6.44 (1), 5.46 (2)"]
["EER","","","","6.29 (1), 3.84 (2)","6.29 (1), 3.84 (2)","5.72 (1), 3.72 (2)","5.72 (1), 3.72 (2)","5.51 (1), 3.61 (2)","5.51 (1), 3.61 (2)"]
["Heating capacity","Nom.","","kW","4.07 (1), 4.33 (2)","4.07 (1), 4.33 (2)","5.86 (1), 6.06 (2)","5.86 (1), 6.06 (2)","7.20 (1), 7.66 (2)","7.20 (1), 7.66 (2)"]
["Power input","Heating","Nom.","kW","0.830 (1), 1.22 (2)","0.830 (1), 1.22 (2)","1.18 (1), 1.73 (2)","1.18 (1), 1.73 (2)","1.61 (1), 2.20 (2)","1.61 (1), 2.20 (2)"]
["","Cooling","Nom.","kW","0.800 (1), 1.16 (2)","0.800 (1), 1.16 (2)","1.07 (1), 1.33 (2)","1.07 (1), 1.33 (2)","1.17 (1), 1.51 (2)","1.17 (1), 1.51 (2)"]
["Notes","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]