{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RKHBRD-ACV1"]
[]
[]
[]
[]
["","","","","RKHBRD011ACV1","RKHBRD014ACV1","RKHBRD016ACV1"]
["Sound pressure level","Nom.","","dBA","43 (5), 46 (6)","45 (5), 46 (6)","46 (5), 46 (6)"]
["Refrigerant","Charge","","kg","2.6","2.6","2.6"]
["","Type","","","R-134a","R-134a","R-134a"]
["Dimensions","Unit","Width","mm","600","600","600"]
["","","Depth","mm","695","695","695"]
["","","Height","mm","705","705","705"]
["Casing","Material","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["","Colour","","","Metallic grey","Metallic grey","Metallic grey"]
["Weight","Unit","","kg","144","144","144"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","V1","V1","V1"]
["","Frequency","","Hz","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240"]
["Current","Recommended fuses","","A","25","25","25"]
["Notes","","","","(1) - Nominal water flow rate for Dt: 10°C","(1) - Nominal water flow rate for Dt: 10°C","(1) - Nominal water flow rate for Dt: 10°C"]
["","","","","(2) - Maximum water flow rate for Dt: 5°C","(2) - Maximum water flow rate for Dt: 5°C","(2) - Maximum water flow rate for Dt: 5°C"]
["","","","","(3) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections.","(3) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections.","(3) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections."]
["","","","","(4) - Values are sound pressure values measured at all sides (front, back, left, right, top) at 1m distance. The values do not occur simultaneously on all mentioned sides.","(4) - Values are sound pressure values measured at all sides (front, back, left, right, top) at 1m distance. The values do not occur simultaneously on all mentioned sides.","(4) - Values are sound pressure values measured at all sides (front, back, left, right, top) at 1m distance. The values do not occur simultaneously on all mentioned sides."]
["","","","","(5) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(5) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(5) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB"]
["","","","","(6) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(6) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(6) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB"]
["","","","","(7) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(7) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(7) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase"]
["","","","","(8) - Zmax: In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax","(8) - Zmax: In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax","(8) - Zmax: In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax"]
["","","","","(9) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A.","(9) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A.","(9) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A."]