{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RKXYQ-T8"]
[]
[]
[]
[]
["","","","","RKXYQ5T8Y1B"]
["Sound pressure level","Cooling","Nom.","dBA","47.0 (5)"]
["Standard Accessories","Installation and operation manual","","","1"]
["","Connection pipes","","","4"]
["","Declaration of conformity","","","1"]
["","Refrigerant label for F-gas regulation","","","1"]
["","Tie-wraps","","","3"]
["","Screws","","","1"]
["Compressor","Type","","","Hermetically sealed swing compressor"]
["Weight","Unit","","kg","79"]
["Refrigerant","GWP","","","2,087.5"]
["","Charge","","kg","2.00"]
["","Type","","","R-410A"]
["Sound power level","Cooling","Nom.","dBA","60.0 (4)"]
["Dimensions","Unit","Width","mm","600"]
["","","Depth","mm","554"]
["","","Height","mm","701"]
["Power supply","Phase","","","3N~"]
["","Name","","","Y1"]
["","Frequency","","Hz","50"]
["","Voltage","","V","380-415"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%)."]
["","","","","(4) - Sound power level is an absolute value that a sound source generates."]
["","","","","(5) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","(6) - Refer to refrigerant pipe selection or installation manual"]
["","","","","(7) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","(8) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current."]
["","","","","(9) - In accordance with EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply wih Ssc  ≥ minimum Ssc value"]
["","","","","(10) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current."]
["","","","","(11) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","(12) - TOCA means the total value of each OC set."]
["","","","","(13) - FLA means the nominal running current of the fan"]
["","","","","(14) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(15) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(16) - Sound values are measured in a semi-anechoic room."]
["","","","","(17) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","(18) - Ssc: Short-circuit power"]
["","","","","(19) - For detailed contents of standard accessories, see installation/operation manual"]