{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RPS"]
[]
[]
[]
[]
["","","","","RPS4"]
["Stand still temperature","Max.","","°C","85"]
["Dimensions","Unit","Width","mm","142"]
["","","Depth","mm","230"]
["","","Height","mm","815"]
["Weight","Unit","","kg","6"]
["Operation range","Ambient temperature","Max.","°C","40"]
["","","Min.","°C","5"]
["Mounting","","","","On side of tank"]
["Power supply intake","","","","Indoor unit"]
["Control","Type","","","Digital temperature difference controller with plain text display"]
["","Power consumption","","W","2"]
["Power supply","Phase","","","1~"]
["","Frequency","","Hz","50"]
["","Voltage","","V","230"]