{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":8,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RRRQ-AY1"]
[]
[]
[]
[]
["","","","","","RRRQ011AAY1","RRRQ014AAY1","RRRQ016AAY1"]
["Sound pressure level","Heating","","Nom.","dBA","","53","55"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","9.4","9.4"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","4.5","4.5"]
["","Type","","","","","R-410A","R-410A"]
["Operation range","Heating","","Max.","°CWB","","20","20"]
["","","","Min.","°CWB","","-20","-20"]
["","Domestic hot water","","Min.","°CDB","","-20","-20"]
["","","","Max.","°CDB","","35","35"]
["Piping connections","Heat insulation","","","","","Both liquid and gas pipes","Both liquid and gas pipes"]
["","Liquid","","OD","mm","","9.52","9.52"]
["","Gas","","OD","mm","","15.9","15.9"]
["","Drain","","OD","mm","","26x3","26x3"]
["","Level difference","IU - OU","Max.","m","","30","30"]
["Sound power level","Heating","","Nom.","dBA","","69","71"]
["Dimensions","Unit","","Width","mm","","900","900"]
["","","","Depth","mm","","320","320"]
["","","","Height","mm","","1,345","1,345"]
["Weight","Unit","","","kg","","120","120"]
["Power supply","Phase","","","","","3~","3~"]
["","Name","","","","","Y1","Y1"]
["","Frequency","","","Hz","","50","50"]
["","Voltage","","","V","","380-415","380-415"]
["Current","Recommended fuses","","","A","","16","16"]
["Notes","","","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","","","(2) - Contains fluorinated greenhouse gases","(2) - Contains fluorinated greenhouse gases"]
["","","","","","","(3) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current less than or equal to 75A","(3) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current less than or equal to 75A"]
["Dimensions","Unit","","Height","mm","1345"]
["","","","Width","mm","900"]
["","","","Depth","mm","320"]
["Weight","Unit","","","kg","120"]
["Operation range","Heating","","Min.","°CWB","-20"]
["","","","Max.","°CWB","20"]
["","Domestic hot water","","Min.","°CDB","-20"]
["","","","Max.","°CDB","35"]
["Sound power level","Heating","","Nom.","dBA","68"]
["Sound pressure level","Heating","","Nom.","dBA","52"]
["Refrigerant","Type","","","","R-410A"]
["","GWP","","","","2087.5"]
["","Charge","","","tCO2Eq","9.4"]
["","Charge","","","kg","4.5"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","15.9"]
["","Drain","","OD","mm","26x3"]
["","Level difference","IU - OU","Max.","m","30"]
["","Heat insulation","","","","Both liquid and gas pipes"]
["Power supply","Name","","","","Y1"]
["","Phase","","","","3~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Current","Recommended fuses","","","A","16"]