{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-A"]
[]
[]
[]
[]
["","","","","","RXC25AV1B","RXC35AV1B","RXC50AV1B","RXC60AV1B"]
["Sound pressure level","Cooling","","High","dBA","","46","","51"]
["Standard Accessories","Drain joint","","","","Drain joint","Drain joint","Drain joint","Drain joint"]
["","Drain plug","","","","Drain plug","Drain plug","Drain plug","Drain plug"]
["Refrigerant","Charge","","","TCO2Eq","","0.54","","0.81"]
["","GWP","","","","","675","","675"]
["","Charge","","","kg","","0.80","","1.20"]
["","Type","","","","","R-32","","R-32"]
["Piping connections","Level difference","IU - OU","Max.","m","","15","","15"]
["","Additional refrigerant charge","","","kg/m","","0,017 (for piping length exceeding 7.5m)","","0,017 (for piping length exceeding 7.5m)"]
["Dimensions","Unit","","Width","mm","","658","","855"]
["","","","Depth","mm","","289","","328"]
["","","","Height","mm","","550","","753"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","","26","","44"]
["Power supply","Phase","","","","","1~","","1~"]
["","Frequency","","","Hz","","50","","50"]
["","Voltage","","","V","","220-240","","220-240"]
["Notes","","","","","","(1) - Contains fluorinated greenhouse gases","","(1) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","550","","628"]
["","","","Width","mm","658","","855"]
["","","","Depth","mm","289","","328"]
["Weight","Unit","","","kg","24","","41"]
["Compressor","Type","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","10","","-10"]
["","","","Max.","°CDB","46","","46"]
["","Heating","Ambient","Min.","°CWB","-15","","-15"]
["","","","Max.","°CWB","18","","18"]
["Sound pressure level","Cooling","","High","dBA","45","","51"]
["Refrigerant","Type","","","","R-32","","R-32"]
["","Charge","","","kg","0.6","","1.1"]
["","Charge","","","tCO2Eq","0.41","","0.74"]
["","GWP","","","","675","","675"]
["Piping connections","Piping length","OU - IU","Max.","m","20","","30"]
["","Additional refrigerant charge","","","kg/m","0,017 (for piping length exceeding 7.5m)","","0,017 (for piping length exceeding 7.5m)"]
["","Level difference","IU - OU","Max.","m","15","","15"]
["Power supply","Phase","","","","1~","","1~"]
["","Frequency","","","Hz","50","","50"]
["","Voltage","","","V","220-240","","220-240"]