{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":80,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SP-O"]
[]
[]
[]
[]
["","","","","","SB.BSP110P1D","SB.BSP110P2D","SB.BSP110P3D","SB.BSP112P1D","SB.BSP112P2D","SB.BSP112P3D","SB.BSP117P1D","SB.BSP117P2D","SB.BSP117P3D","SB.BSP218P1D","SB.BSP218P2D","SB.BSP218P3D","SB.BSP220P1D","SB.BSP220P2D","SB.BSP220P3D","SB.BSP330P1D","SB.BSP330P2D","SB.BSP330P3D","SB.MSP106P1E","SB.MSP106P2E","SB.MSP106P3E","SB.MSP107P1E","SB.MSP107P2E","SB.MSP107P3E","SB.MSP212P1E","SB.MSP212P2E","SB.MSP212P3E","SB.MSP213P1E","SB.MSP213P2E","SB.MSP213P3E","SB.MSP315P1E","SB.MSP315P2E","SB.MSP315P3E","SB.MSP320P1E","SB.MSP320P2E","SB.MSP320P3E","MSP106EA12XXA","MSP106EA12XXB","MSP107EA12XXA","MSP107EA12XXB","BSP110DA12XXA","BSP110DA12XXB","BSP112DA12XXA","BSP112DA12XXB","BSP117DA12XXA","BSP117DA12XXB","SB.BSP121NO488D","SB.BSP121TO488D","SB.MSP121TO488E","SB.BSP123TO488D","SB.MSP123TO488E","SB.BSP135TO479D","SB.MSP135NO479E","MSP212EB12XXA","MSP212EB12XXB","MSP212EA12XXA","MSP212EA12XXB","MSP213EB12XXA","MSP213EB12XXB","BSP218DA12XXA","BSP218DA12XXB","BSP220DB12XXA","BSP220DB12XXB","SB.BSP221NO488D","SB.MSP221NO488E","SB.BSP221TO479D","SB.MSP221TO479E","MSP315EB13XXA","MSP315EB13XXB","MSP320EB13XXA","MSP320EB13XXB","BSP320DB13XXA","BSP320DB13XXB","BSP330DB13XXA","BSP330DB13XXB"]
["Refrigerant","GWP","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","2,141","2,141","1,430","2,141","1,430","2,141","1,430","","","","","","","","","","","2,141","1,430","2,141","1,430"]
["","Type","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","R-134a","","R-134a","","R-134a","","","","","","","","","","","","R-134a","","R-134a"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","1.140 (1)","","1.422 (1)","","3.188 (1)","","","","","","","","","","","","1.816 (1)","","2.029 (1)"]
["","Low temperature","R-452A","Nom","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","0.662 (1)","0.905 (1)","","1.088 (1)","","2.384 (1)","","","","","","","","","","","","1.342 (1)","","1.719 (1)"]
["Operation range","Cold room temperature","","Min.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","-25","-25","-5","-25","-5","-25","-5","","","","","","","","","","","-25","-5","-25","-5"]
["","","","Max.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","-15","-15","10","-15","10","-15","10","","","","","","","","","","","-15","10","-15","10"]
["Defrost","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","Electric","Electric","Electric","Electric","Electric","Electric","","","Electric","","Electric","","Electric","","Electric","","Electric","Electric","Electric","Electric","Electric","","Electric","","Electric","","Electric"]
["Dimensions","Evaporator unit","","Depth","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","410","410","410","410","410","410","410","","","","","","","","","","","410","410","410","410"]
["","","","Height","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","215","215","215","215","215","215","215","","","","","","","","","","","215","215","215","215"]
["","","","Width","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","614","614","614","614","614","1,614","1,614","","","","","","","","","","","1,034","1,034","1,034","1,034"]
["","Condensing unit","","Depth","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","337","337","337","337","337","427","427","","","","","","","","","","","427","427","427","427"]
["","","","Width","mm","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","620","620","620","620","620","820","820","","","","","","","","","","","820","820","820","820"]
["Compressor","Nominal power","","","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","0.75","1.1","0.4","1.3","0.7","2.2","2.2","","","","","","","","","","","1.3","0.9","1.5","1.7"]
["","Type","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","","","","","","","","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating"]
["","Starting method","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","","","","","","","","","","","Direct","Direct","Direct","Direct"]
["Condenser","Air flow","","","m³/h","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","750","750","750","750","750","1,500","1,500","","","","","","","","","","","1,400","1,400","1,400","1,400"]
["Evaporator","Air flow","","","m³/h","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","600","600","600","600","600","1,800","1,800","","","","","","","","","","","1,200","1,200","1,200","1,200"]
["","Air throw","","","m","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","","","","","","","","","","","4 (2)","4 (2)","4 (2)","4 (2)"]
["Defrost heaters","W","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","450","","450","","450","","450","","450","","450","450","450","450","450","1,400","1,400","","","800","","800","","800","","800","","800","800","800","800","1400","","1400","","1400","","1400"]
["Power supply","Phase","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","1~","1~","1~","1~","1~","3N~","3N~","","","","","","","","","","","1~","1~","3N~","3N~"]
["","Frequency","","","Hz","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","50","50","50","50","50","50","50","","","","","","","","","","","50","50","50","50"]
["","Voltage","","","V","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","230","230","230","230","230","400","400","","","","","","","","","","","230","230","400","400"]
["Notes","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","","","","","","","","","","","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C"]
["","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","","","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]
["","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]
["Refrigerating capacity","Low temperature","R-452A","Nom","kW","0.662","0.662","0.662","0.905","0.905","0.905","1.088","1.088","1.088","1.342","1.342","1.342","1.719","1.719","1.719","2.384","2.384","2.384","","","","","","","","","","","","","","","","","","","","","","","0.662","","0.905","","1.164","","","","","","","","","","","","","","","1.436","","1.719","","","","","","","","","","2.384","","2.581"]
["Dimensions","Condensing unit","","Width","mm","620","620","620","620","620","620","620","620","620","820","820","820","820","820","820","820","820","820","620","620","620","620","620","620","820","820","820","820","820","820","820","820","820","820","820","820","660","","660","","660","","660","","660","","","","","","","","","820","","860","","820","","860","","860","","","","","","860","","860","","860","","860"]
["","","","Depth","mm","337","337","337","337","337","337","337","337","337","427","427","427","427","427","427","427","427","427","337","337","337","337","337","337","427","427","427","427","427","427","427","427","427","427","427","427","337","","337","","337","","337","","337","","","","","","","","","427","","427","","427","","427","","427","","","","","","427","","427","","427","","427"]
["","Evaporator unit","","Height","mm","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","215","","215","","215","","215","","215","","215","","","","","","","","","215","","215","","215","","215","","215","","","","","","215","","215","","215","","215"]
["","","","Width","mm","614","614","614","614","614","614","614","614","614","1034","1034","1034","1034","1034","1034","1614","1614","1614","614","614","614","614","614","614","1034","1034","1034","1034","1034","1034","1614","1614","1614","1614","1614","1614","","654","","654","","654","","654","","654","","","","","","","","","1034","","1074","","1034","","1074","","1074","","","","","","1654","","1654","","1654","","1654"]
["","","","Depth","mm","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","410","","410","","410","","410","","410","","410","","","","","","","","","410","","410","","410","","410","","410","","","","","","410","","410","","410","","410"]
["Compressor","Type","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","","","","","","","","Hermetic Reciprocating","","Hermetic","","Hermetic Reciprocating","","Hermetic","","Hermetic","","","","","","Hermetic","","Hermetic","","Hermetic","","Hermetic"]
["","Starting method","","","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","Direct","","Direct","","Direct","","Direct","","Direct","","","","","","","","","Direct","","Direct","","Direct","","Direct","","Direct","","","","","","Direct","","Direct","","Direct","","Direct"]
["Condenser","Air flow","","","m³/h","750","750","750","750","750","750","750","750","750","1400","1400","1400","1400","1400","1400","1500","1500","1500","750","750","750","750","750","750","1400","1400","1400","1400","1400","1400","1500","1500","1500","1500","1500","1500","750","","750","","750","","750","","750","","","","","","","","","1400","","1400","","1400","","1400","","1400","","","","","","1500","","1500","","1500","","1500"]
["Power supply","Voltage","","","V","230","230","230","230","230","230","230","230","230","230","230","230","400","400","400","400","400","400","230","230","230","230","230","230","230","230","230","400","400","400","400","400","400","400","400","400","220-230","","220-230","","220-230","","220-230","","220-230","","","","","","","","","230","","220-230","","400","","220-230","","380-400","","","","","","380-400","","380-400","","380-400","","380-400"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","3N~","3N~","3N~","3N~","3N~","3N~","1~","1~","1~","1~","1~","1~","1~","1~","1~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","1~","","1~","","1~","","1~","","1~","","","","","","","","","1~","","1~","","3N~","","1~","","3N~","","","","","","3N~","","3N~","","3N~","","3N~"]
["Refrigerant","Type","","","","","","","","","","R-452A","R-452A","R-452A","R-452A","R-452A","R-452A","R-452A","R-452A","R-452A","R-452A","R-452A","R-452A","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","R-134a","","R-134a","","R-452A","","R-452A","","R-452A","","","","","","","","","R-134a","","R-134a","","R-134a","","R-452A","","R-452A","","","","","","R-134a","","R-134a","","R-452A","","R-452A"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","","","","","","","","","","","","","","","","","","1.14","1.14","1.14","1.422","1.422","1.422","1.816","1.816","1.816","2.029","2.029","2.029","3.188","3.188","3.188","3.492","3.492","3.492","1.14","","1.422","","","","","","","","","","","","","","","1.816","","1.816","","2.029","","","","","","","","","","3.188","","3.492"]
["Casing","Colour","","Condensing unit","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","White","White","White","White","White","White","White","White","White","White","","","","","","","","","","White","White","","","White","White","White","White","","","","","White","White","White","White","White","White","White","White"]
["Compressor","Quantity","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","1","","1","","1","","1","","1","","","","","","","","","","","1","","","","1","","1","","","","","","1","","1","","1","","1"]
["","Model","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","NJ6220Z","","NTU6222ZV","","NEU2178GK","","NJ2192GK","","NJ2212GK","","","","","","","","","","","FH4518Y/F","","","","NJ2212GK","","TFH2480Z/T","","","","","","TFH4525Y/T","","MTZ40JH4","","TFH2511Z","","NTZ068A4LR1B"]
["Operation range","Cold room temperature","","Min.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","-5","","-5","","-25","","-25","","-25","","","","","","","","","","","-5","","-5","","-25","","-25","","","","","","-5","","-5","","-25","","-25"]
["","","","Max.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","10","","10","","-15","","-15","","-15","","","","","","","","","","","10","","10","","-15","","-15","","","","","","10","","10","","-15","","-15"]
["","Ambient temperature","","Min.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","20","","20","","20","","20","","20","","","","","","","","","","","20","","","","20","","20","","","","","","20","","20","","20","","20"]
["","","","Max.","°C","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","45","","45","","45","","45","","45","","","","","","","","","","","45","","","","45","","45","","","","","","45","","45","","45","","45"]
["Refrigerant","GWP","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","1430","","1430","","2140","","2140","","2140","","","","","","","","","","","1430","","1430","","2140","","2140","","","","","","1430","","1430","","2140","","2140"]
["Power supply","Frequency","","","Hz","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","50","","50","","50","","50","","50","","","","","","","","","","","50","","50","","50","","50","","","","","","50","","50","","50","","50"]
["Evaporator","Air throw","","","m","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","4","","4","","4","","4","","4","","","","","","","","","","","4","","4 (2)","","4","","4","","","","","","4","","4","","4","","4"]
["Notes","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","(1) - When normally running: 0°C / +30°C","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]